<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<eagle version="9.5.1">
<drawing>
<library>
<packages>
<package name="LOGO-PYR0BALL-SS-6MM"/>
<package name="MICRO-USB5+6P-SMD-0.65-AB">
</package>
<package name="R0402">
</package>
<package name="MICRO-USB5+4P-SMD-0.65-B">
</package>
<package name="DO-214AA">
</package>
<package name="SJW">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJM">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="AMPHENOL_10118192-0001LF">
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="DO41-7.6">
<description>&lt;b&gt;DO41&lt;/b&gt; 7.6mm x 2mm&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
</package>
<package name="QFN50P500X500X80-29N">
</package>
<package name="22-23-2031">
<description>&lt;b&gt;KK® 254 Solid Header, Vertical, with Friction Lock, 3 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022232031_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="82114R">
<description>&lt;B&gt;INDUCTOR&lt;/B&gt;&lt;p&gt;
manufacturer Siemens</description>
</package>
<package name="SOT89">
</package>
<package name="PIEZO-DISK-20MM">
</package>
<package name="PIEZO-DISK-12MM">
</package>
<package name="SOT230P700X180-4N">
</package>
<package name="HDRVR4W64P254_1X4_1016X254X575B">
<description>Single-row, 4-pin Receptacle Header (Female) Straight, 2.54 mm (0.10 in) col pitch, 5.75 mm insulator length, 10.16 X 2.54 X 5.75 mm body
&lt;p&gt;Single-row (1X4), 4-pin Receptacle Header (Female) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.75 mm insulator length with overall size 10.16 X 2.54 X 5.75 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="TO18">
<description>&lt;b&gt;TO 18&lt;/b&gt;</description>
</package>
<package name="KK-156-2">
<description>&lt;b&gt;KK® 396 Header, Vertical, Friction Lock, 2 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/026604020_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="FFC-60P_0.5_MOLEX_505110-6091">
<description>&lt;b&gt;0.5mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
</package>
<package name="TO18-">
<description>&lt;b&gt;TO-18&lt;/b&gt;</description>
</package>
<package name="TO3">
<description>&lt;b&gt;TO-3&lt;/b&gt;</description>
</package>
<package name="SOT93V">
<description>SOT-93&lt;p&gt;
grid 5.45 mm</description>
</package>
<package name="SOT93">
<description>SOT-93&lt;p&gt;
grid 5.45 mm</description>
</package>
<package name="TO126">
<description>&lt;b&gt;TO 126 horizontal&lt;/b&gt;</description>
</package>
<package name="TO18V">
<description>&lt;b&gt;TO-18&lt;/b&gt;</description>
</package>
<package name="TO218V">
<description>&lt;b&gt;TO 218 vertical&lt;/b&gt;</description>
</package>
<package name="TO202">
<description>&lt;b&gt;TO 202 horizontal&lt;/b&gt;</description>
</package>
<package name="TO39">
<description>&lt;b&gt;TO-39&lt;/b&gt;</description>
</package>
<package name="TO126V">
<description>&lt;b&gt;TO 126 vertical&lt;/b&gt;</description>
</package>
<package name="TO5">
<description>&lt;b&gt;TO 5&lt;/b&gt;</description>
</package>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line E B C from top&lt;p&gt;</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="TO218">
<description>&lt;b&gt;TO 218 horizontal&lt;/b&gt;</description>
</package>
<package name="SOT89-ECB">
<description>SOT89 Emitter Collector Basis</description>
</package>
<package name="TO202V">
<description>&lt;b&gt;TO 202 vertical&lt;/b&gt;</description>
</package>
<package name="TOP3">
<description>&lt;b&gt;TOP 3 horizontal&lt;/b&gt;</description>
</package>
<package name="TO92-CBE">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line  C B E from top&lt;p&gt;</description>
</package>
<package name="TO92-CEB">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line C E B from top&lt;p&gt;</description>
</package>
<package name="SC59-BEC">
<description>SC59 (SOT23) Motorola</description>
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 220 vertical&lt;/b&gt;</description>
</package>
<package name="TO92-BCE">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line B C E from top&lt;p&gt;</description>
</package>
<package name="TO92-BEC">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line  B E C from top&lt;p&gt;</description>
</package>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
<package name="TO66">
<description>&lt;b&gt;TO-66&lt;/b&gt;</description>
</package>
<package name="TO225AA">
<description>&lt;b&gt;TO-225&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, vertical</description>
</package>
<package name="TO92-E1">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads Triangle Reverse</description>
</package>
<package name="SOT23-EBC">
<description>&lt;b&gt;SOT-23 (EBC)&lt;/b&gt;</description>
</package>
<package name="TOP3V">
<description>&lt;b&gt;TOP 3 vertical&lt;/b&gt;</description>
</package>
<package name="TO92L">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="TO92/">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 2.54 mm&lt;p&gt;
rotated 45 deg.</description>
</package>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
<package name="SOT89-BCE">
<description>SOT89 Basis Collector Emitter</description>
</package>
<package name="CAPC1005X50">
<description>Chip, 1.00 X 0.55 X 0.50 mm body
&lt;p&gt;Chip package with body size 1.00 X 0.55 X 0.50 mm&lt;/p&gt;</description>
</package>
<package name="DO-219AC">
</package>
<package name="SOT23-BCE">
<description>&lt;b&gt;SOT-23 (BCE)&lt;/b&gt;</description>
</package>
<package name="FID_060">
<description>Fiducial 60mil</description>
</package>
<package name="FID_020_P">
<description>Fiducial 20mil with paste for alignment</description>
</package>
<package name="FID_040">
<description>Fiducial 40mil</description>
</package>
<package name="FID_020">
<description>Fiducial 20mil</description>
</package>
<package name="FID_060_P">
<description>Fiducial 60mil with paste for alignment</description>
</package>
<package name="FFC-15P-1MM">
</package>
<package name="FID_040_P">
<description>Fiducial 40mil with paste for alignment</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOIC127P789X216-8N">
</package>
<package name="70553-04">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Low Profile, Single Row, Right Angle, 3.05mm Pocket, Shrouded, 5 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705530004_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="70543-04">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Single Row, Vertical, 3.05mm Pocket, Shrouded, 5 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705430004_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="74099-04">
<description>&lt;b&gt;SL™ Wire-to-Board Header, Surface Mount, Single Row, Vertical, 3.05mm Pocket, Shrouded, 4 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705530004_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="15-91-04">
<description>&lt;b&gt;2.54mm Pitch SL™ Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg, 4 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/015913044_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="CAPC2012X130">
<description>Chip, 2.00 X 1.25 X 1.30 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.25 X 1.30 mm&lt;/p&gt;</description>
</package>
<package name="HDRVR5W64P254_1X5_1270X254X575B">
<description>Single-row, 5-pin Receptacle Header (Female) Straight, 2.54 mm (0.10 in) col pitch, 5.75 mm insulator length, 12.70 X 2.54 X 5.75 mm body
&lt;p&gt;Single-row (1X5), 5-pin Receptacle Header (Female) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.75 mm insulator length with overall size 12.70 X 2.54 X 5.75 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="1X2MTA">
<description>&lt;b&gt;AMP MTA connector&lt;/b&gt;</description>
</package>
<package name="7395-04">
<description>&lt;b&gt;KK® 254 Wire-to-Board Header, Right Angle, with Friction Lock, 4 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022057048_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="6410-04">
<description>&lt;b&gt;KK® 254 Wire-to-Board Header, Vertical, with Friction Lock, 4 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022272041_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="STA_RAVF164-M">
</package>
<package name="EXBN8V-L">
</package>
<package name="STA_RAVF164">
</package>
<package name="EXBN8V-M">
</package>
<package name="STA_RAVF164-L">
</package>
<package name="CAPC1609X80">
<description>Chip, 1.60 X 0.90 X 0.80 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.90 X 0.80 mm&lt;/p&gt;</description>
</package>
<package name="EXBN8V">
</package>
<package name="SILABS_QFN20">
</package>
<package name="53261-02">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Surface Mount, Right Angle, 2 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/532610271_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="MICROSWITCH_5.08">
</package>
<package name="SEEED-RESISTOR_R0603">
</package>
<package name="53398-02">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Surface Mount, Vertical, 2 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/533980271_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="SOT143">
</package>
<package name="53047-02">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Wire-to-Board Header, Vertical, with Friction Lock, 2 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/530470210_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="53048-02">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Right Angle, 2 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/530480210_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="ICSP_3X2_2X1.5_SPRING_CONTACTS">
<description>Three-row, 6-pin Pin Header (Male) Straight, 2.00 mm (0.08 in) row pitch, 2.00 mm (0.08 in) col pitch, 4.00 mm mating length, 4.00 X 6.00 X 5.50 mm body
&lt;p&gt;Three-row (3X2), 6-pin Pin Header (Male) Straight package with 2.00 mm (0.08 in) row pitch, 2.00 mm (0.08 in) col pitch, 0.50 mm lead width, 2.60 mm tail length and 4.00 mm mating length with overall size 4.00 X 6.00 X 5.50 mm, pin pattern - counter-clockwise from bottom left&lt;/p&gt;</description>
</package>
<package name="ICSP_3X2_2.54_STRAIGHT">
<description>Three-row, 6-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 5.08 X 7.62 X 8.38 mm body
&lt;p&gt;Three-row (3X2), 6-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.84 mm mating length with overall size 5.08 X 7.62 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="ICSP_3X2_3.48X1.1_SPRING_CONTACTS">
<description>Three-row, 6-pin Pin Header (Male) Straight, 2.00 mm (0.08 in) row pitch, 2.00 mm (0.08 in) col pitch, 4.00 mm mating length, 4.00 X 6.00 X 5.50 mm body
&lt;p&gt;Three-row (3X2), 6-pin Pin Header (Male) Straight package with 2.00 mm (0.08 in) row pitch, 2.00 mm (0.08 in) col pitch, 0.50 mm lead width, 2.60 mm tail length and 4.00 mm mating length with overall size 4.00 X 6.00 X 5.50 mm, pin pattern - counter-clockwise from bottom left&lt;/p&gt;</description>
</package>
<package name="ICSP_2X3_2.54_RIGHT">
<description>Double-row, 6-pin Pin Header (Male) Right Angle, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 7.62 X 2.54 X 5.08 mm body
&lt;p&gt;Double-row (2X3), 6-pin Pin Header (Male) Right Angle package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.84 mm mating length with body size 7.62 X 2.54 X 5.08 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="QFN50P500X500X100-33N">
</package>
<package name="ICSP_3X2_2MM_STRAIGHT">
<description>Three-row, 6-pin Pin Header (Male) Straight, 2.00 mm (0.08 in) row pitch, 2.00 mm (0.08 in) col pitch, 4.00 mm mating length, 4.00 X 6.00 X 5.50 mm body
&lt;p&gt;Three-row (3X2), 6-pin Pin Header (Male) Straight package with 2.00 mm (0.08 in) row pitch, 2.00 mm (0.08 in) col pitch, 0.50 mm lead width, 2.60 mm tail length and 4.00 mm mating length with overall size 4.00 X 6.00 X 5.50 mm, pin pattern - counter-clockwise from bottom left&lt;/p&gt;</description>
</package>
<package name="SC70">
<description>&lt;b&gt;SC70-3 Reflow soldering&lt;/b&gt;&lt;p&gt;
Philips SC01_Mounting_1996.pdf&lt;p&gt;
ROHM : UMT3 ; EIAJ : SC-70</description>
</package>
<package name="SOT-563">
</package>
<package name="SEEED-SWITCH_SW2-2.6-3.0X2.5X1.2+0.4MM">
</package>
<package name="QFN50P500X500X90-33N">
</package>
<package name="53261-03">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Surface Mount, Right Angle, 3 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/532610371_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="FH12-40S-0.5SH">
<description>&lt;b&gt;0.5mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
</package>
<package name="53047-03">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Wire-to-Board Header, Vertical, with Friction Lock, 3 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/530470310_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="53048-03">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Right Angle, 3 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/530480310_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="B6">
<description>Becher B6 (cup B6)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 16x11
RM (grid) [mm]: 8.75x10 / 5x12.5
manufactured by NKL®</description>
</package>
<package name="SMD">
<description>SMD     top view
ca. Maße (approx. dim.)[mm]:
LxB(W)xH : 17x13x7
pad: 2.8x1.8</description>
</package>
<package name="QFN50P700X700X90-49N">
</package>
<package name="S11-10">
<description>Sockel S11 (base S11)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 12x6x12
RM (grid) [mm]: 7.5
manufactured by NKL®</description>
</package>
<package name="B5">
<description>Becher B5 (cup B5)   top view
ca. Maße (approx. dimensions):
LxB(W)xH [mm]: 13x6x14
RM (grid): (10x3)mm
manufactured by NKL®</description>
</package>
<package name="QFN16">
<description>&lt;b&gt;RTE (S-PQFP-N16)&lt;/b&gt; 3x3 mm&lt;p&gt;&#xD;
Source: www.ti.com .. tpa6132a2 direct path stereo $.65.pdf</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SEEED-SWITCH_SW6-2.54-9.0X3.5X3.2+2.0MM">
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="SSOP14">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
<package name="22-23-2021">
<description>&lt;b&gt;KK® 254 Solid Header, Vertical, with Friction Lock, 2 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022232021_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
<package name="LSU260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
1 mm, round, Siemens</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="Q62902-B152">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="LED2X5">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
2 x 5 mm, rectangle</description>
</package>
<package name="Q62902-B156">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="SFH482">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="LZR181">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
1 LED, Siemens</description>
</package>
<package name="OSRAM-SIDELED">
<description>&lt;b&gt;Super SIDELED® High-Current LED&lt;/b&gt;&lt;p&gt;
LG A672, LP A672 &lt;br&gt;
Source: http://www.osram.convergy.de/ ... LG_LP_A672.pdf (2004.05.13)</description>
</package>
<package name="Q62902-B155">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="U57X32">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
rectangle, 5.7 x 3.2 mm</description>
</package>
<package name="MICRO-SIDELED">
<description>&lt;b&gt;Hyper Micro SIDELED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY Y876.pdf</description>
</package>
<package name="SMART-LED">
<description>&lt;b&gt;SmartLEDTM Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY L896.pdf</description>
</package>
<package name="Q62902-B153">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="SFH480">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="IRL80A">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
IR transmitter Siemens</description>
</package>
<package name="LED10MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
10 mm, round</description>
</package>
<package name="LUMILED">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; without cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
<package name="P-LCC-2-TOPLED-RG">
<description>&lt;b&gt;Hyper TOPLED® RG Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY T776.pdf</description>
</package>
<package name="P-LCC-2">
<description>&lt;b&gt;TOPLED® High-optical Power LED (HOP)&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... ls_t675.pdf</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="SMARTLED-TTW">
<description>&lt;b&gt;SmartLED TTW&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="OSRAM-MINI-TOP-LED">
<description>&lt;b&gt;BLUE LINETM Hyper Mini TOPLED® Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LB M676.pdf</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="LUMILED+">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; with cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="KA-3528ASYC">
<description>&lt;b&gt;SURFACE MOUNT LED LAMP&lt;/b&gt; 3.5x2.8mm&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/KA-3528ASYC(Ver1189474662.1)</description>
</package>
<package name="MINI-TOPLED-SANTANA">
<description>&lt;b&gt;Mini TOPLED Santana®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG M470.pdf</description>
</package>
<package name="FUSE_0402">
<description>Chip, 1.00 X 0.50 X 0.39 mm body
&lt;p&gt;Chip package with body size 1.00 X 0.50 X 0.39 mm&lt;/p&gt;</description>
</package>
<package name="HOLES_2,8-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, round</description>
</package>
<package name="SML1206">
<description>&lt;b&gt;SML10XXKH-TR (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;SML10R3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10E3KH-TR&lt;/td&gt;&lt;td&gt;SUPER REDSUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10O3KH-TR&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PY3KH-TR&lt;/td&gt;&lt;td&gt;PURE YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10OY3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10AG3KH-TR&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10BG3KH-TR&lt;/td&gt;&lt;td&gt;BLUE GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PB1KH-TR&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10CW1KH-TR&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;

Source: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF</description>
</package>
<package name="HOLES_3,2-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.2 mm, round</description>
</package>
<package name="53398-03">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Surface Mount, Vertical, 3 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/533980371_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="HOLES_4,3-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.3 mm, round</description>
</package>
<package name="HOLES_5,5-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 5.5 mm, round</description>
</package>
<package name="HOLES_3,3-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.3 mm, round</description>
</package>
<package name="HOLES_5,0-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 5.0 mm, round</description>
</package>
<package name="HOLES_4,1-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.1 mm, round</description>
</package>
<package name="HOLES_3,6-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.6 mm, round</description>
</package>
<package name="HOLES_3,0-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.0 mm, round</description>
</package>
<package name="HDRRAR4W64P254_2X2_556X736X556B">
<description>Double-row, 4-pin Receptacle Header (Female) Right Angle, 2.54 mm (0.10 in) pitch, 7.36 mm insulator length, 5.56 X 7.36 X 5.56 mm body
&lt;p&gt;Double-row (2X2), 4-pin Receptacle Header (Female) Right Angle package with 2.54 mm (0.10 in) pitch, 0.64 mm lead width, 3.00 mm tail length and 7.36 mm insulator length with body size 5.56 X 7.36 X 5.56 mm, pin pattern - counter-clockwise from bottom left&lt;/p&gt;</description>
</package>
<package name="SOT-23-5_MC-M">
</package>
<package name="SOT-23-5_MC-L">
</package>
<package name="SOT-23-5_MC">
</package>
<package name="HOLES_4,5-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.5 mm, round</description>
</package>
<package name="MCS08">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.2 mm</description>
</package>
<package name="4PLCC">
</package>
<package name="SEEED-LED_LED-0603">
</package>
<package name="TRIM_TC33X-2-103E">
<description>&lt;b&gt;3 mm SMD Trimming Potentiometer&lt;/b&gt; Side Adjust&lt;p&gt;
Source: http://www.bourns.com/data/global/PDFs/3223.PDF</description>
</package>
<package name="0606_LED">
<description>&lt;h3&gt;0606 - LED SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.8mm&lt;/li&gt;
&lt;li&gt;Area:1.6mm L x 1.5mm W&lt;/li&gt;
&lt;li&gt;Height: 0.55m&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://optoelectronics.liteon.com/upload/download/DS22-2000-282/P_100_LTST-C195KGJRKT.pdf"&gt;LTST-C195KGJRKT&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LTST-C195KGJRKT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="28M1">
</package>
<package name="28M1-M">
</package>
<package name="LOGO-PYR0BALL-IMPRESSION">
</package>
<package name="70553-03">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Low Profile, Single Row, Right Angle, 3.05mm Pocket, Shrouded, 4 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705530003_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="15-91-03">
<description>&lt;b&gt;2.54mm Pitch SL™ Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg, 3 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/015913034_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="74099-03">
<description>&lt;b&gt;SL™ Wire-to-Board Header, Surface Mount, Single Row, Vertical, 3.05mm Pocket, Shrouded, 3 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705530003_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="70543-03">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Single Row, Vertical, 3.05mm Pocket, Shrouded, 4 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705430003_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="CON24_1X24_DRB_SFW">
</package>
<package name="DO-214AC">
<description>&lt;b&gt;SURFACE MOUNT GENERAL RECTIFIER&lt;/b&gt; JEDEC DO-214AC molded platic body&lt;p&gt;
Method 2026&lt;br&gt;
Source: http://www.kingtronics.com/SMD_M7/M7_SMD_4007.pdf</description>
</package>
<package name="LOGO-PYR0BALL-EMBOSS-35MM">
</package>
<package name="LOGO-PYR0BALL-EMBOSS-15MM">
</package>
<package name="8-POWERTDFN">
</package>
<package name="28M1-L">
</package>
<package name="LOGO-PYR0BALL-SS-20MM">
</package>
<package name="LOGO-PYR0BALL">
</package>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="SC-74-6">
</package>
<package name="DIOC1006X70">
<description>Chip, 1.00 X 0.60 X 0.70 mm body
&lt;p&gt;Chip package with body size 1.00 X 0.60 X 0.70 mm&lt;/p&gt;</description>
</package>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="PW8">
</package>
<package name="PW8-M">
</package>
<package name="PW8-L">
</package>
<package name="53398-06">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Surface Mount, Vertical, 6 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/533980671_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="CAPPRD254W65D650H1250B">
<description>Radial Polarized Capacitor, 2.54 mm pitch, 6.50 mm body diameter, 12.50 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 2.54 mm pitch, 0.65 mm lead diameter, 6.50 mm body diameter and 12.50 mm body height&lt;/p&gt;</description>
</package>
<package name="SON50P200X200X60-9N">
</package>
<package name="ALU-C-D5.3MM_RIGHT">
</package>
<package name="ALU-C-D5.3MM_LEFT">
</package>
<package name="53048-06">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Right Angle, 6 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/530480610_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="53261-04">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Surface Mount, Right Angle, 4 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/532610471_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="53047-06">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Wire-to-Board Header, Vertical, with Friction Lock, 6 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/530470610_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="PP-STANDALONE-HEADER">
<description>Double-row, 12-pin Receptacle Header (Female) Right Angle, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 7.36 mm insulator length, 15.24 X 7.36 X 5.56 mm body
&lt;p&gt;Double-row (2X6), 12-pin Receptacle Header (Female) Right Angle package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 7.36 mm insulator length with body size 15.24 X 7.36 X 5.56 mm, pin pattern - counter-clockwise from bottom left&lt;/p&gt;</description>
</package>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="53398-04">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Surface Mount, Vertical, 4 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/533980471_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="53047-04">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Wire-to-Board Header, Vertical, with Friction Lock, 4 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/530470410_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="P1-13Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-17Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-17">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP07SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP07R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP09R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-20Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP11R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-20">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP10SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP06SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP13R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP18R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP09SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP15SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP06R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP08R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP18SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="1X3MTA">
<description>&lt;b&gt;AMP MTA connector&lt;/b&gt;</description>
</package>
<package name="TP14SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP08SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP12SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP14R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP11SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP17SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP10R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP15R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP16R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP12R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP16SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP13SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP13SQ-HOLE">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP19SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP19R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="SPRING_CONTACT_2.5X1.5">
<description>Spring loaded contact
https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10104320.pdf</description>
</package>
<package name="SPRING_CONTACT_3.48X1.10">
<description>Spring loaded contact
https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10104320.pdf</description>
</package>
<package name="SOP65P490X110-8N">
</package>
<package name="QFN45P300X300X85-21N">
</package>
<package name="15-91-02">
<description>&lt;b&gt;2.54mm Pitch SL™ Wire-to-Board Header, Low Profile, Surface Mount, Single Row, Right Angle, 3.05mm Pocket, Shrouded, with Press-fit Plastic Peg, 2 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/015913024_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="TP17R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="70553-02">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Low Profile, Single Row, Right Angle, 3.05mm Pocket, Shrouded, 3 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705530002_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="70543-02">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Single Row, Vertical, 3.05mm Pocket, Shrouded, 3 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705430002_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="53261-06">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Surface Mount, Right Angle, 6 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/532610671_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="53048-04">
<description>&lt;b&gt;1.25mm Pitch PicoBlade™ Header, Right Angle, 4 Circuits&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/530480410_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
</packages>
<symbols>
<symbol name="LED-RG">
<description>&lt;h3&gt;RG LED - No Common&lt;/h3&gt;
&lt;p&gt;4 pin RG LED&lt;/p&gt;</description>
<pin name="GC" direction="pas"/>
<pin name="GA" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="RA" direction="pas"/>
</symbol>
<symbol name="LM358_PW_8">
<pin name="1OUT" direction="out"/>
<pin name="1IN-" direction="in"/>
<pin name="1IN+" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="2IN+" direction="in"/>
<pin name="2IN-" direction="in"/>
<pin name="2OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="RES2">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="ZX62-B-5PA(11)">
<description>&lt;b&gt;ZX62-B-5PA(11)&lt;/b&gt;&lt;br&gt;
Hirose Micro-USB B connector&lt;br&gt;
SMD type&lt;br&gt;</description>
<pin name="VBUS" direction="sup"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="ID"/>
<pin name="GND" direction="sup"/>
<pin name="SHIELD" direction="sup"/>
</symbol>
<symbol name="LM358QT">
<pin name="OUT1" direction="out"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="VCC-" direction="pwr"/>
<pin name="IN2+" direction="in"/>
<pin name="IN2-" direction="in"/>
<pin name="OUT2" direction="out"/>
<pin name="VCC+" direction="pwr"/>
<pin name="EXP" direction="pwr"/>
</symbol>
<symbol name="RGB_COM_CATH">
<pin name="RED"/>
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="CAT"/>
</symbol>
<symbol name="USB-MICRO-5P">
<pin name="VCC"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="ID"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
</symbol>
<symbol name="RES1">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="10118192-0001LF">
<pin name="VUSB" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="ID" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="RES">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="CP2102N-A01-GQFN28">
<pin name="GPIO.1/RXT"/>
<pin name="GPIO.0/TXT"/>
<pin name="GND" direction="pwr"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREGIN" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="!RST" direction="in"/>
<pin name="!SUSPENDB" direction="out"/>
<pin name="CHREN" direction="out"/>
<pin name="SUSPEND" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="GPIO.2/RS485"/>
<pin name="GPIO.3/WAKEUP"/>
<pin name="DSR" direction="in"/>
<pin name="DTR" direction="out"/>
<pin name="DCD" direction="in"/>
<pin name="RI/CLK"/>
<pin name="CHR1" direction="out"/>
<pin name="CHR0" direction="out"/>
<pin name="GPIO.6"/>
<pin name="GPIO.4"/>
<pin name="GPIO.5"/>
</symbol>
<symbol name="SCHOTTKY-1">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SJ">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="L78L05ACU">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="PAD" direction="pwr"/>
</symbol>
<symbol name="M-6">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="DRK">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="MV-6">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="SEEED-CONNECTOR_HEADER-4P">
<pin name="P$1" function="dotclk"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
</symbol>
<symbol name="LM317DCY">
<pin name="INPUT" direction="in"/>
<pin name="ADJUST" direction="in"/>
<pin name="OUTPUT_2" direction="out"/>
<pin name="OUTPUT" direction="out"/>
</symbol>
<symbol name="PIEZO-SMD">
<pin name="GND" direction="pas"/>
<pin name="PZ+"/>
</symbol>
<symbol name="MV-3">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="CON-2X30+SHIELD">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="52" direction="pas"/>
<pin name="53" direction="pas"/>
<pin name="54" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="56" direction="pas"/>
<pin name="57" direction="pas"/>
<pin name="58" direction="pas"/>
<pin name="59" direction="pas"/>
<pin name="60" direction="pas"/>
<pin name="61" direction="pas"/>
<pin name="62" direction="pas"/>
<pin name="63" direction="pas"/>
<pin name="64" direction="pas"/>
<pin name="65" direction="pas"/>
<pin name="66" direction="pas"/>
<pin name="S@1" direction="pas"/>
<pin name="S@2" direction="pas"/>
</symbol>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PNP-1">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="D-ZENER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="NPN-2">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="FIDUCIAL">
<description>Empty symbol so a blank device can be made. Sometimes when working with scripts and ULPs they error when there are board-only elements</description>
</symbol>
<symbol name="RES-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="ATTINY85V-10SH">
<pin name="VCC" direction="pwr"/>
<pin name="PB5"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="GND" direction="pas"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
</symbol>
<symbol name="FFC-15P-1MM">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
</symbol>
<symbol name="NPN-1">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="M">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="KA2KA">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="AC" direction="pas"/>
</symbol>
<symbol name="SEEED-CAPACITOR_C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MV">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MTA-02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JST-2.54MM_HEADER-5P">
<pin name="P$1" function="dotclk"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
</symbol>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="TP">
<pin name="TP" direction="in"/>
</symbol>
<symbol name="SEEED-RESISTOR_RES">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CP2102N-A01-GQFN20">
<pin name="GPIO.1/RS485"/>
<pin name="GPIO.0/CLK"/>
<pin name="GND" direction="pwr"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREGIN" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="RST" direction="in" function="dot"/>
<pin name="NC" direction="nc"/>
<pin name="SUSPENDB" direction="out" function="dot"/>
<pin name="WAKEUP" direction="in"/>
<pin name="SUSPEND" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="GPIO.3/RXT"/>
<pin name="GPIO.2/TXT"/>
</symbol>
<symbol name="SPDT_SWITCH">
<pin name="COM"/>
<pin name="NC"/>
<pin name="NO"/>
</symbol>
<symbol name="SP0503BAHTG">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="MV-1">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="M-1">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="ATMEGA328PB-MU_PWR">
<pin name="GND0" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="PAD" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ICSP">
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="RST"/>
<pin name="GND" direction="pwr"/>
<pin name="MOSI"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ATMEGA328PB-MU">
<pin name="PD3/OC2B/INT1/PTCXY"/>
<pin name="PD4/XCK0/T0/PTCXY"/>
<pin name="PE0/SDA1/ICP4/ACO/PTCXY"/>
<pin name="PE1/SCL1/T4/PTCXY"/>
<pin name="PB6/XTAL1/TOSC1"/>
<pin name="PB7/XTAL2/TOSC2"/>
<pin name="PD5/OC0B/T1/PTCXY"/>
<pin name="PD6/OC0A/PTCXY/AIN0"/>
<pin name="PD7/PTCXY/AIN1"/>
<pin name="PB0/ICP1/CLKO/PTCXY"/>
<pin name="PB1/OC1A/PTCXY"/>
<pin name="PB2/!SS0!/OC1B/PTCXY"/>
<pin name="PB3/MOSI0/TXD1/OC2A/PTCXY"/>
<pin name="PB4/MISO0/RXD1/PTCXY"/>
<pin name="PB5/PTCXY/XCK1/SCK0"/>
<pin name="PE2/ADC6/PTCY/ICP3/!SS1!"/>
<pin name="AREF" direction="in"/>
<pin name="PE3/ADC7/PTCY/T3/MOSI1"/>
<pin name="PC0/ADC0/PTCY/MISO1"/>
<pin name="PC1/ADC1/PTCY/SCK1"/>
<pin name="PC2/ADC2/PTCY"/>
<pin name="PC3/ADC3/PTCY"/>
<pin name="PC4/ADC4/PTCY/SDA0"/>
<pin name="PC5/ADC5/PTCY/SCL0"/>
<pin name="PC6/!RESET!"/>
<pin name="PD0/PTCXY/OC3A/RXD0"/>
<pin name="PD1/PTCXY/OC4A/TXD0"/>
<pin name="PD2/PTCXY/INT0/OC3B/OC4B"/>
</symbol>
<symbol name="LEVEL_SHIFT_NCH_MOSFET">
<pin name="D"/>
<pin name="S"/>
<pin name="G"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="ATSAMD21E18A-MU">
<pin name="PA00"/>
<pin name="PA01"/>
<pin name="PA02"/>
<pin name="PA03"/>
<pin name="VDDANA" direction="pwr"/>
<pin name="PA04"/>
<pin name="PA05"/>
<pin name="PA06"/>
<pin name="PA07"/>
<pin name="PA08"/>
<pin name="PA09"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="GND" direction="pwr"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PA16"/>
<pin name="PA17"/>
<pin name="PA18"/>
<pin name="PA19"/>
<pin name="PA22"/>
<pin name="PA23"/>
<pin name="PA24"/>
<pin name="PA25"/>
<pin name="PA27"/>
<pin name="!RESET" direction="in"/>
<pin name="PA28"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="VDDIN" direction="pwr"/>
<pin name="PA30"/>
<pin name="PA31"/>
<pin name="EP" direction="pwr"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SEEED-SWITCH_BUTTON-2P">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="MV-2">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PINV">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PIN">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="M-2">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="OPAMP-1">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="ATSAM3S4AA-MU_GPIO">
<pin name="PB0/AD4"/>
<pin name="PB1/AD5"/>
<pin name="PB2/AD6"/>
<pin name="PB3/AD7"/>
<pin name="PA17/PGMD5/AD0"/>
<pin name="PA18/PGMD6/AD1"/>
<pin name="PA19/PGMD7/AD2"/>
<pin name="PA20/AD3"/>
<pin name="PA16/PGMD4"/>
<pin name="PA15/PGMD3"/>
<pin name="PA14/PGMD2"/>
<pin name="PA13/PGMD1"/>
<pin name="PA12/PGMD0"/>
<pin name="PA11/PGMM3"/>
<pin name="PA10/PGMM2"/>
<pin name="PA9/PGMM1"/>
<pin name="PA8/XOUT32/PGMM0"/>
<pin name="PA7/XIN32/PGMNVALID"/>
<pin name="TDI/PB4"/>
<pin name="PA6/PGMNOE"/>
<pin name="PA5/PGMRDY"/>
<pin name="PA4/PGMNCMD"/>
<pin name="NRST"/>
<pin name="PA3"/>
<pin name="PA2/PGMEN2"/>
<pin name="PA1/PGMEN1"/>
<pin name="PA0/PGMEN0"/>
<pin name="PB5/TDO/TRACESWO"/>
<pin name="JTAGEL"/>
<pin name="PB6/TMS/SWDIO"/>
<pin name="PB7/TCK/SWCLK"/>
<pin name="ERASE/PB12"/>
<pin name="PB10/DDM"/>
<pin name="PB11/DDP"/>
<pin name="XOUT/PB8"/>
<pin name="XIN/PB9/GMCK"/>
<pin name="TST"/>
<pin name="ADVREFP"/>
</symbol>
<symbol name="SINGLE">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="ATSAM4N8AA-MU_PWR">
<pin name="GND0"/>
<pin name="VDDIN"/>
<pin name="VDDOUT"/>
<pin name="VDDIO0"/>
<pin name="VDDCORE0"/>
<pin name="VDDIO1"/>
<pin name="GND1"/>
<pin name="VDDCORE1"/>
<pin name="VDDIO2"/>
<pin name="VDDPLL"/>
<pin name="PAD"/>
</symbol>
<symbol name="SEEED-SWITCH_SWITCH-2CH-6P">
<pin name="CH1A"/>
<pin name="CH1B"/>
<pin name="CH2A"/>
<pin name="CH2B"/>
<pin name="COM1" function="dot"/>
<pin name="COM2" function="dotclk"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="M-3">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="FUSE">
<pin name="P$1" direction="pwr"/>
<pin name="P$2" direction="pwr"/>
</symbol>
<symbol name="HOLES_MOUNT-PAD">
<pin name="MOUNT" direction="pas"/>
</symbol>
<symbol name="LED-1">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="MCP6001T-I/OT">
<pin name="VOUT" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="VIN+" direction="pas"/>
<pin name="VIN-" direction="pas"/>
<pin name="VDD" direction="pas"/>
</symbol>
<symbol name="TC33X-2-103E">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SEEED-LED_LED-1">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="RGB_COM_ANO">
<pin name="RED"/>
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="ANO"/>
</symbol>
<symbol name="LSP">
<pin name="MP" direction="pas"/>
</symbol>
<symbol name="ATMEGA48PA-MMHR_A">
<pin name="AVCC" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND_2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ATMEGA48PA-MMHR">
<pin name="(PCINT19/OC2B/INT1)_PD3"/>
<pin name="(PCINT20/XCK/T0)_PD4"/>
<pin name="(PCINT21/OC0B/T1)_PD5"/>
<pin name="(PCINT22/OC0A/AIN0)_PD6"/>
<pin name="(PCINT23/AIN1)_PD7"/>
<pin name="29" direction="pas"/>
<pin name="AREF" direction="pas"/>
<pin name="PB5_(SCK/PCINT5)"/>
<pin name="PD0_(RXD/PCINT16)"/>
<pin name="PD1_(TXD/PCINT17)"/>
<pin name="PD2_(INT0/PCINT18)"/>
<pin name="(PCINT0/CLKO/ICP1)_PB0"/>
<pin name="(PCINT1/OC1A)_PB1"/>
<pin name="(PCINT2/SS/OC1B)_PB2"/>
<pin name="(PCINT3/OC2A/MOSI)_PB3"/>
<pin name="(PCINT4/MISO)_PB4"/>
<pin name="(PCINT6/XTAL1/TOSC1)_PB6"/>
<pin name="(PCINT7/XTAL2/TOSC2)_PB7"/>
<pin name="PC0_(ADC0/PCINT8)"/>
<pin name="PC1_(ADC1/PCINT9)"/>
<pin name="PC2_(ADC2/PCINT10)"/>
<pin name="PC3_(ADC3/PCINT11)"/>
<pin name="PC4_(ADC4/SDA/PCINT12)"/>
<pin name="PC5_(ADC5/SCL/PCINT13)"/>
<pin name="PC6_(RESET/PCINT14)"/>
</symbol>
<symbol name="LOGO-PYR0BALL">
</symbol>
<symbol name="ATSAM4N8AA-MU_GPIO">
<pin name="PB0/AD4"/>
<pin name="PB1/AD5"/>
<pin name="PB2/AD6"/>
<pin name="PB3/AD7"/>
<pin name="PA17/PGMD5/AD0"/>
<pin name="PA18/PGMD6/AD1"/>
<pin name="PA19/PGMD7/AD2"/>
<pin name="PA20/AD3"/>
<pin name="PA16/PGMD4"/>
<pin name="PA15/PGMD3"/>
<pin name="PA14/PGMD2"/>
<pin name="PA13/PGMD1"/>
<pin name="PA12/PGMD0"/>
<pin name="PA11/PGMM3"/>
<pin name="PA10/PGMM2"/>
<pin name="PA9/PGMM1"/>
<pin name="PA8/XOUT32/PGMM0"/>
<pin name="PA7/XIN32/PGMNVALID"/>
<pin name="TDI/PB4"/>
<pin name="PA6/PGMNOE"/>
<pin name="PA5/PGMRDY"/>
<pin name="PA4/PGMNCMD"/>
<pin name="NRST"/>
<pin name="PA3"/>
<pin name="PA2/PGMEN2"/>
<pin name="PA1/PGMEN1"/>
<pin name="PA0/PGMEN0"/>
<pin name="PB5/TDO/TRACESWO"/>
<pin name="JTAGEL"/>
<pin name="PB6/TMS/SWDIO"/>
<pin name="PB7/TCK/SWCLK"/>
<pin name="ERASE/PB12"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="XOUT/PB8"/>
<pin name="XIN/PB9/GMCK"/>
<pin name="TST"/>
<pin name="ADVREFP"/>
</symbol>
<symbol name="TVS_DIODE_CHANNEL">
<pin name="CH$1"/>
</symbol>
<symbol name="CON24_1X24_DRB_SFW">
<pin name="11" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="55" direction="pas"/>
<pin name="66" direction="pas"/>
<pin name="77" direction="pas"/>
<pin name="88" direction="pas"/>
<pin name="99" direction="pas"/>
<pin name="1010" direction="pas"/>
<pin name="1111" direction="pas"/>
<pin name="1212" direction="pas"/>
<pin name="1313" direction="pas"/>
<pin name="1414" direction="pas"/>
<pin name="1515" direction="pas"/>
<pin name="1616" direction="pas"/>
<pin name="1717" direction="pas"/>
<pin name="1818" direction="pas"/>
<pin name="1919" direction="pas"/>
<pin name="2020" direction="pas"/>
<pin name="2121" direction="pas"/>
<pin name="2222" direction="pas"/>
<pin name="2323" direction="pas"/>
<pin name="2424" direction="pas"/>
<pin name="2525" direction="pas"/>
<pin name="2626" direction="pas"/>
</symbol>
<symbol name="TVS_DIODE_PRIMARY">
<pin name="CH$1"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="CAP-POLAR">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="OPAMP+GN">
<pin name="1IN-" direction="in"/>
<pin name="1IN+" direction="in"/>
<pin name="1OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="OPAMP">
<pin name="2IN-" direction="in"/>
<pin name="2IN+" direction="in"/>
<pin name="2OUT" direction="out"/>
</symbol>
<symbol name="MV-5">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="M-5">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MV-4">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PP-STANDALONE-PWM">
<pin name="FOL_PWM"/>
<pin name="COMP_PWM"/>
</symbol>
<symbol name="PP-STANDALONE-SENSE">
<pin name="FOL_S"/>
<pin name="COMP_S"/>
</symbol>
<symbol name="PP-STANDALONE-POWER">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PP-STANDALONE-GADJ">
<pin name="GADG_R0"/>
<pin name="GADG_R1"/>
<pin name="GADG_R2"/>
<pin name="GADG_R3"/>
</symbol>
<symbol name="PP-STANDALONE-OUTPUT">
<pin name="Z-TRG"/>
<pin name="PT100"/>
</symbol>
<symbol name="MTA-03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="ATTINY84A-MMH">
<pin name="VCC" direction="pwr"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="GND_2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="DNC_2" direction="nc"/>
<pin name="DNC_3" direction="nc"/>
<pin name="DNC_4" direction="nc"/>
<pin name="DNC_5" direction="nc"/>
<pin name="DNC_6" direction="nc"/>
<pin name="DNC" direction="nc"/>
</symbol>
<symbol name="M-4">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MCP6232T-E/MS">
<pin name="VINA-" direction="in"/>
<pin name="VINA+" direction="in"/>
<pin name="VINB-" direction="in"/>
<pin name="VINB+" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pas"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-0R-5%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010000</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402JR-070RL"/>
<attribute name="VALUE" value="0R"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10118192-0001LF" prefix="J">
<description>Single Port 5 Contact Horizontal Right Angle Shielded Micro B USB 2.0 Connector</description>
<gates>
<gate name="G$1" symbol="10118192-0001LF"/>
</gates>
<devices>
<device name="" package="AMPHENOL_10118192-0001LF">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="SH1 SH2 SH3 SH4 SH5 SH6"/>
<connect gate="G$1" pin="VUSB" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value=" Conn Micro USB Type B RCP 5 POS 0.65mm Solder RA SMD 5 Terminal 1 Port T/R "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="609-4613-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/amphenol-fci/10118192-0001LF/609-4613-1-ND/2785378?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Amphenol FCI"/>
<attribute name="MP" value="10118192-0001LF"/>
<attribute name="PACKAGE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SJ" prefix="SJ" uservalue="yes">
<description>SMD solder &lt;b&gt;JUMPER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="SJ"/>
</gates>
<devices>
<device name="" package="SJ">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SJW">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SJM">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP2102N-A01-GQFN28" prefix="U">
<description>Ic Bridge Usb To Uart 28qfn</description>
<gates>
<gate name="G$1" symbol="CP2102N-A01-GQFN28"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X80-29N">
<connects>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="!SUSPENDB" pad="11"/>
<connect gate="G$1" pin="CHR0" pad="15"/>
<connect gate="G$1" pin="CHR1" pad="14"/>
<connect gate="G$1" pin="CHREN" pad="13"/>
<connect gate="G$1" pin="CTS" pad="23"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="5"/>
<connect gate="G$1" pin="DCD" pad="1"/>
<connect gate="G$1" pin="DSR" pad="27"/>
<connect gate="G$1" pin="DTR" pad="28"/>
<connect gate="G$1" pin="GND" pad="3 29"/>
<connect gate="G$1" pin="GPIO.0/TXT" pad="19"/>
<connect gate="G$1" pin="GPIO.1/RXT" pad="18"/>
<connect gate="G$1" pin="GPIO.2/RS485" pad="17"/>
<connect gate="G$1" pin="GPIO.3/WAKEUP" pad="16"/>
<connect gate="G$1" pin="GPIO.4" pad="22"/>
<connect gate="G$1" pin="GPIO.5" pad="21"/>
<connect gate="G$1" pin="GPIO.6" pad="20"/>
<connect gate="G$1" pin="RI/CLK" pad="2"/>
<connect gate="G$1" pin="RTS" pad="24"/>
<connect gate="G$1" pin="RXD" pad="25"/>
<connect gate="G$1" pin="SUSPEND" pad="12"/>
<connect gate="G$1" pin="TXD" pad="26"/>
<connect gate="G$1" pin="VBUS" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VREGIN" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Usb-Uart Interface Bridge, Qfn-28 "/>
<attribute name="MF" value="Silicon Labs"/>
<attribute name="MP" value="CP2102N-A01-GQFN28"/>
<attribute name="PACKAGE" value="QFN-28 Silicon Labs"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82114R" prefix="L">
<description>&lt;B&gt;INDUCTOR&lt;/B&gt;</description>
<gates>
<gate name="1" symbol="DRK"/>
</gates>
<devices>
<device name="" package="82114R">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="L"/>
</technology>
</technologies>
</device>
</devices>
<spice>
<pinmapping spiceprefix="L">
<pinmap gate="1" pin="1" pinorder="1"/>
<pinmap gate="1" pin="2" pinorder="2"/>
</pinmapping>
</spice>
</deviceset>
<deviceset name="SCHOTTKY_1N5819" prefix="D">
<description>&lt;b&gt;1.0A SCHOTTKY BARRIER RECTIFIER&lt;/b&gt;&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY-1"/>
</gates>
<devices>
<device name="" package="DO41-7.6">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="7-B"/>
<technology name="7-T"/>
<technology name="8-B"/>
<technology name="8-T"/>
<technology name="9-B"/>
<technology name="9-T"/>
</technologies>
</device>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L78L05ACU">
<description>5V Positive voltage regulator SMD SOT89 Package</description>
<gates>
<gate name="G$1" symbol="L78L05ACU"/>
</gates>
<devices>
<device name="" package="SOT89">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="PAD" pad="PAD"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Voltage regulator; fixed; 5V; 0.1A; SOT89; SMD; Package: reel, tape "/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MP" value="L78L05ACU-TR"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIEZO-DISK" prefix="PZ">
<gates>
<gate name="G$1" symbol="PIEZO-SMD"/>
</gates>
<devices>
<device name="12MM" package="PIEZO-DISK-12MM">
<connects>
<connect gate="G$1" pin="GND" pad="GND1 GND2 GND3 GND4"/>
<connect gate="G$1" pin="PZ+" pad="PZ+" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20MM" package="PIEZO-DISK-20MM">
<connects>
<connect gate="G$1" pin="GND" pad="GND1 GND2 GND3 GND4"/>
<connect gate="G$1" pin="PZ+" pad="PZ+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22-23-2031" prefix="X">
<description>.100" (2.54mm) Center Header - 3 Pin</description>
<gates>
<gate name="-1" symbol="MV-6"/>
<gate name="-2" symbol="M-6"/>
<gate name="-3" symbol="M-6"/>
</gates>
<devices>
<device name="" package="22-23-2031">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="OC_NEWARK" value="30C0862"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CONNECTOR_DIP-BLACK-FEMALE-HEADER-VERT(4P-2.54)" prefix="J" uservalue="yes">
<description>320030017</description>
<gates>
<gate name="G$1" symbol="SEEED-CONNECTOR_HEADER-4P"/>
</gates>
<devices>
<device name="JST-2.54MM_4P" package="HDRVR4W64P254_1X4_1016X254X575B">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM317DCY" prefix="U">
<description>IC ADJ LINEAR REG 1.25V TO 37V</description>
<gates>
<gate name="A" symbol="LM317DCY"/>
</gates>
<devices>
<device name="" package="SOT230P700X180-4N">
<connects>
<connect gate="A" pin="ADJUST" pad="1"/>
<connect gate="A" pin="INPUT" pad="3"/>
<connect gate="A" pin="OUTPUT" pad="4"/>
<connect gate="A" pin="OUTPUT_2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" IC Regulator LM317/SOT223/LM317DCY TEXAS INSTRUMENT RoHS Ampere=1.5 SOT223 "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="LM317DCY"/>
<attribute name="PACKAGE" value="SOT-223-4 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FFC_MOLEX_0.5MM" prefix="J">
<gates>
<gate name="G$1" symbol="CON-2X30+SHIELD"/>
</gates>
<devices>
<device name="" package="FFC-60P_0.5_MOLEX_505110-6091">
<connects>
<connect gate="G$1" pin="10" pad="8"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="10"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="12"/>
<connect gate="G$1" pin="15" pad="13"/>
<connect gate="G$1" pin="16" pad="14"/>
<connect gate="G$1" pin="17" pad="15"/>
<connect gate="G$1" pin="18" pad="16"/>
<connect gate="G$1" pin="19" pad="17"/>
<connect gate="G$1" pin="20" pad="18"/>
<connect gate="G$1" pin="21" pad="19"/>
<connect gate="G$1" pin="22" pad="20"/>
<connect gate="G$1" pin="23" pad="21"/>
<connect gate="G$1" pin="24" pad="22"/>
<connect gate="G$1" pin="25" pad="23"/>
<connect gate="G$1" pin="26" pad="24"/>
<connect gate="G$1" pin="27" pad="25"/>
<connect gate="G$1" pin="28" pad="26"/>
<connect gate="G$1" pin="29" pad="27"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="30" pad="28"/>
<connect gate="G$1" pin="31" pad="29"/>
<connect gate="G$1" pin="32" pad="30"/>
<connect gate="G$1" pin="37" pad="31"/>
<connect gate="G$1" pin="38" pad="32"/>
<connect gate="G$1" pin="39" pad="33"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="40" pad="34"/>
<connect gate="G$1" pin="41" pad="35"/>
<connect gate="G$1" pin="42" pad="36"/>
<connect gate="G$1" pin="43" pad="37"/>
<connect gate="G$1" pin="44" pad="38"/>
<connect gate="G$1" pin="45" pad="39"/>
<connect gate="G$1" pin="46" pad="40"/>
<connect gate="G$1" pin="47" pad="41"/>
<connect gate="G$1" pin="48" pad="42"/>
<connect gate="G$1" pin="49" pad="43"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="50" pad="44"/>
<connect gate="G$1" pin="51" pad="45"/>
<connect gate="G$1" pin="52" pad="46"/>
<connect gate="G$1" pin="53" pad="47"/>
<connect gate="G$1" pin="54" pad="48"/>
<connect gate="G$1" pin="55" pad="49"/>
<connect gate="G$1" pin="56" pad="50"/>
<connect gate="G$1" pin="57" pad="51"/>
<connect gate="G$1" pin="58" pad="52"/>
<connect gate="G$1" pin="59" pad="53"/>
<connect gate="G$1" pin="6" pad="4"/>
<connect gate="G$1" pin="60" pad="54"/>
<connect gate="G$1" pin="61" pad="55"/>
<connect gate="G$1" pin="62" pad="56"/>
<connect gate="G$1" pin="63" pad="57"/>
<connect gate="G$1" pin="64" pad="58"/>
<connect gate="G$1" pin="65" pad="59"/>
<connect gate="G$1" pin="66" pad="60"/>
<connect gate="G$1" pin="7" pad="5"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="7"/>
<connect gate="G$1" pin="S@1" pad="S$1"/>
<connect gate="G$1" pin="S@2" pad="S$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KK-156-2" prefix="X" uservalue="yes">
<description>&lt;b&gt;KK 156 HEADER&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com/pdm_docs/sd/026604100_sd.pdf</description>
<gates>
<gate name="-1" symbol="MV-3"/>
<gate name="-2" symbol="MV-3"/>
</gates>
<devices>
<device name="" package="KK-156-2">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N2907" prefix="T">
<description>&lt;b&gt;NPN TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="TO92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N3904" prefix="T">
<description>&lt;b&gt;NPN TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="G1" symbol="NPN-1"/>
</gates>
<devices>
<device name="" package="TO92">
<connects>
<connect gate="G1" pin="B" pad="2"/>
<connect gate="G1" pin="C" pad="1"/>
<connect gate="G1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N2222" prefix="T">
<description>&lt;b&gt;NPN TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="NPN-2"/>
</gates>
<devices>
<device name="" package="TO18">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-1NF-50V-10%-X7R(0402)" prefix="C" uservalue="yes">
<description>302010005</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="CAP_0402" package="CAPC1005X50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_ZENER_PLZ5V1C" prefix="D">
<gates>
<gate name="G$1" symbol="D-ZENER"/>
</gates>
<devices>
<device name="" package="DO-219AC">
<connects>
<connect gate="G$1" pin="A" pad="P$1"/>
<connect gate="G$1" pin="C" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*-PNP-" prefix="T" uservalue="yes">
<description>PNP Transistror</description>
<gates>
<gate name="G$1" symbol="PNP-1"/>
</gates>
<devices>
<device name="TO3" package="TO3">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO18-EBC" package="TO18">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name="2N2906"/>
<technology name="2N2906A"/>
<technology name="2N2907"/>
<technology name="2N2907A"/>
<technology name="2N3251"/>
<technology name="2N3963"/>
<technology name="BC177B"/>
<technology name="BC393"/>
<technology name="BCY70"/>
<technology name="BCY79-IX"/>
<technology name="BCY79-VII"/>
<technology name="BCY79-VIII"/>
<technology name="BSS74"/>
<technology name="BSS75"/>
<technology name="BSS76"/>
</technologies>
</device>
<device name="TO18-" package="TO18-">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO18V" package="TO18V">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO202" package="TO202">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO202V" package="TO202V">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT93" package="SOT93">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT93V" package="SOT93V">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO126" package="TO126">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO126V" package="TO126V">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO218" package="TO218">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO218V" package="TO218V">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO220" package="TO220">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO220V" package="TO220V">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO225AA" package="TO225AA">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO39-EBC" package="TO39">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name="2N2904"/>
<technology name="2N2904A"/>
<technology name="2N2905"/>
<technology name="2N2905A"/>
<technology name="2N3467"/>
<technology name="2N3635"/>
<technology name="2N3637"/>
<technology name="2N4033"/>
<technology name="2N5415"/>
<technology name="2N5416"/>
<technology name="BC160-16"/>
<technology name="BC161-16"/>
<technology name="MM4001"/>
</technologies>
</device>
<device name="TO5" package="TO5">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO66" package="TO66">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92-EBC" package="TO92-EBC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="BC327"/>
<technology name="BC327-16"/>
<technology name="BC327-25"/>
<technology name="BC327-40"/>
<technology name="BC328"/>
<technology name="BC328-16"/>
<technology name="BC328-25"/>
<technology name="BC328-40"/>
<technology name="BC448"/>
<technology name="BC450"/>
<technology name="BC488"/>
<technology name="BC490"/>
<technology name="BC516"/>
<technology name="BC556A"/>
<technology name="BC556B"/>
<technology name="BC557A"/>
<technology name="BC557B"/>
<technology name="BC557C"/>
<technology name="BC558A"/>
<technology name="BC558B"/>
<technology name="BC558C"/>
<technology name="BC559A"/>
<technology name="BC559B"/>
<technology name="BC559C"/>
<technology name="BC560C"/>
<technology name="BCX58"/>
<technology name="BCX59"/>
<technology name="BCX79"/>
<technology name="MPSA92"/>
<technology name="MPSA93"/>
</technologies>
</device>
<device name="TO92-E1" package="TO92-E1">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92/" package="TO92/">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92L" package="TO92L">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOP3" package="TOP3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOP3V" package="TOP3V">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23-BEC" package="SOT23-BEC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="BC807-16"/>
<technology name="BC807-16LT1"/>
<technology name="BC807-25"/>
<technology name="BC807-25LT1"/>
<technology name="BC807-40"/>
<technology name="BC807-40LT1"/>
<technology name="BC808-16"/>
<technology name="BC808-25"/>
<technology name="BC856A"/>
<technology name="BC856ALT1"/>
<technology name="BC856B"/>
<technology name="BC856BLT1"/>
<technology name="BC857A"/>
<technology name="BC857ALT1"/>
<technology name="BC857B"/>
<technology name="BC857BLT1"/>
<technology name="BC857C"/>
<technology name="BC858A"/>
<technology name="BC858ALT1"/>
<technology name="BC858B"/>
<technology name="BC858BLT1"/>
<technology name="BC858C"/>
<technology name="BC858CLT1"/>
<technology name="BF821"/>
<technology name="BF823"/>
<technology name="MMBT2907ALT1"/>
<technology name="MMBT3640LT1"/>
<technology name="MMBT3906LT1"/>
<technology name="MMBT4403LT1"/>
<technology name="MMBT540LT1"/>
<technology name="MMBT6520LT1"/>
<technology name="MMBTA92LT1"/>
<technology name="MMBTH81LT1"/>
</technologies>
</device>
<device name="SOT23-EBC" package="SOT23-EBC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT89-ECB" package="SOT89-ECB">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92-BCE" package="TO92-BCE">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="2SC1815"/>
<technology name="BC369"/>
<technology name="BC636"/>
<technology name="BC638"/>
<technology name="BC640"/>
<technology name="BF421"/>
<technology name="BF423"/>
<technology name="MPSA56"/>
</technologies>
</device>
<device name="TO92-CBE" package="TO92-CBE">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="2N4126"/>
<technology name="BF493S"/>
<technology name="MPS2907A"/>
<technology name="MPSA63"/>
<technology name="MPSA64"/>
<technology name="MPSW92"/>
</technologies>
</device>
<device name="TO92-BEC" package="TO92-BEC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92-CEB" package="TO92-CEB">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
<technology name="BC237"/>
<technology name="BC238"/>
<technology name="BC239"/>
<technology name="BF494"/>
<technology name="BF495"/>
</technologies>
</device>
<device name="SOT23-BCE" package="SOT23-BCE">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT98-BCE" package="SOT89-BCE">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="BF621"/>
<technology name="BF623"/>
</technologies>
</device>
<device name="SC59-BEC" package="SC59-BEC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="MMUN2111LT1"/>
<technology name="MMUN2112LT1"/>
<technology name="MMUN2113LT1"/>
<technology name="MMUN2114LT1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FFC-15P-1MM" prefix="J">
<gates>
<gate name="G$1" symbol="FFC-15P-1MM"/>
<gate name="G$2" symbol="TP"/>
<gate name="G$3" symbol="TP"/>
</gates>
<devices>
<device name="" package="FFC-15P-1MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
<connect gate="G$2" pin="TP" pad="P$16"/>
<connect gate="G$3" pin="TP" pad="P$17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FID" prefix="FD">
<description>Fiducial marks. Top and Bottom copper with stop mask</description>
<gates>
<gate name="G$2" symbol="FIDUCIAL"/>
</gates>
<devices>
<device name="_20MIL" package="FID_020">
<technologies>
<technology name="">
<attribute name="BOM" value=""/>
</technology>
</technologies>
</device>
<device name="_40MIL" package="FID_040">
<technologies>
<technology name="">
<attribute name="BOM" value=""/>
</technology>
</technologies>
</device>
<device name="_60MIL" package="FID_060">
<technologies>
<technology name="">
<attribute name="BOM" value=""/>
</technology>
</technologies>
</device>
<device name="_20MIL_P" package="FID_020_P">
<technologies>
<technology name="">
<attribute name="BOM" value=""/>
</technology>
</technologies>
</device>
<device name="_40MIL_P" package="FID_040_P">
<technologies>
<technology name="">
<attribute name="BOM" value=""/>
</technology>
</technologies>
</device>
<device name="_60MIL_P" package="FID_060_P">
<technologies>
<technology name="">
<attribute name="BOM" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-2K-5%-1/8W(0805)" prefix="R" uservalue="yes">
<description>301010318</description>
<gates>
<gate name="G$1" symbol="RES-1"/>
</gates>
<devices>
<device name="" package="R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0805JR-072KL"/>
<attribute name="VALUE" value="2K"/>
</technology>
</technologies>
</device>
<device name="R0805" package="R0805">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY85V-10SH" prefix="U">
<description>Atmel 8-bit AVR Microcontroller,SOIC-8</description>
<gates>
<gate name="A" symbol="ATTINY85V-10SH"/>
</gates>
<devices>
<device name="" package="SOIC127P789X216-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="PB0" pad="5"/>
<connect gate="A" pin="PB1" pad="6"/>
<connect gate="A" pin="PB2" pad="7"/>
<connect gate="A" pin="PB3" pad="2"/>
<connect gate="A" pin="PB4" pad="3"/>
<connect gate="A" pin="PB5" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY85V-10SH"/>
<attribute name="OC_FARNELL" value="Unknown"/>
<attribute name="OC_NEWARK" value="68T3815"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="ATMEL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAV199" prefix="D">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
low-leakage double diode</description>
<gates>
<gate name="G$1" symbol="KA2KA"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="AC" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-GRID-04" prefix="X">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 2.54 mm (0.100") pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
</gates>
<devices>
<device name="-70543" package="70543-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-70553" package="70553-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-74099" package="74099-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-15-91" package="15-91-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MTA02-156" prefix="J" uservalue="yes">
<description>&lt;b&gt;AMP connector&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MTA-02"/>
</gates>
<devices>
<device name="" package="1X2MTA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="POPULARITY" value="4"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST-2.54MM_5P-2.54" prefix="J">
<gates>
<gate name="G$1" symbol="JST-2.54MM_HEADER-5P"/>
</gates>
<devices>
<device name="JST_2.54MM_5P_F" package="HDRVR5W64P254_1X5_1270X254X575B">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22-?-04" prefix="J">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 2.54 mm (.1 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
</gates>
<devices>
<device name="05-7048" package="7395-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="27-2041" package="6410-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR_NETWORK_X4" prefix="R">
<gates>
<gate name="A" symbol="RES"/>
<gate name="B" symbol="RES"/>
<gate name="C" symbol="RES"/>
<gate name="D" symbol="RES"/>
</gates>
<devices>
<device name="1206" package="STA_RAVF164">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="RAVF164DJT1K00"/>
<attribute name="VENDOR" value="Stackpole International"/>
</technology>
</technologies>
</device>
<device name="1206_STA_RAVF164-M" package="STA_RAVF164-M">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="RAVF164DJT1K00"/>
<attribute name="VENDOR" value="Stackpole International"/>
</technology>
</technologies>
</device>
<device name="1206_STA_RAVF164-L" package="STA_RAVF164-L">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="RAVF164DJT1K00"/>
<attribute name="VENDOR" value="Stackpole International"/>
</technology>
</technologies>
</device>
<device name="0804" package="EXBN8V">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0804_L" package="EXBN8V-L">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0804_M" package="EXBN8V-M">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_CERAMIC-10UF-25V-10%-X5R(0805)" prefix="C" uservalue="yes">
<description>302010178</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="CAP_0805-3D" package="CAPC2012X130">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CAP_0603-IMP" package="C0603K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CAP_0603_GEN" package="CAPC1609X80">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CAP_0402-GEN" package="CAPC1005X50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP2102N-A01-GQFN20" prefix="U">
<description>Ic Bridge Usb To Uart 20qfn</description>
<gates>
<gate name="G$1" symbol="CP2102N-A01-GQFN20"/>
</gates>
<devices>
<device name="" package="SILABS_QFN20">
<connects>
<connect gate="G$1" pin="CTS" pad="15"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="5"/>
<connect gate="G$1" pin="GND" pad="3 12 21"/>
<connect gate="G$1" pin="GPIO.0/CLK" pad="2"/>
<connect gate="G$1" pin="GPIO.1/RS485" pad="1"/>
<connect gate="G$1" pin="GPIO.2/TXT" pad="20"/>
<connect gate="G$1" pin="GPIO.3/RXT" pad="19"/>
<connect gate="G$1" pin="NC" pad="10"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="RXD" pad="17"/>
<connect gate="G$1" pin="SUSPEND" pad="14"/>
<connect gate="G$1" pin="SUSPENDB" pad="11"/>
<connect gate="G$1" pin="TXD" pad="18"/>
<connect gate="G$1" pin="VBUS" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VREGIN" pad="7"/>
<connect gate="G$1" pin="WAKEUP" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value=" Usb-Uart Interface Bridge, Qfn-20 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="336-3692-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/silicon-labs/CP2102N-A01-GQFN20/336-3692-ND/6012517?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Silicon Labs"/>
<attribute name="MP" value="CP2102N-A01-GQFN20"/>
<attribute name="PACKAGE" value="QFN-20 Silicon Labs"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIMIT_SWITCH" prefix="SW">
<gates>
<gate name="G$1" symbol="SPDT_SWITCH"/>
</gates>
<devices>
<device name="MICRO_SPDT_5.08" package="MICROSWITCH_5.08">
<connects>
<connect gate="G$1" pin="COM" pad="P$1"/>
<connect gate="G$1" pin="NC" pad="P$3"/>
<connect gate="G$1" pin="NO" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-RESISTOR_SMD-RES-1.5K-1%-1/10W(0603)" prefix="R" uservalue="yes">
<description>301010189</description>
<gates>
<gate name="G$1" symbol="SEEED-RESISTOR_RES"/>
</gates>
<devices>
<device name="DETAILED_MODEL" package="SEEED-RESISTOR_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SP0503BAHTG" prefix="D">
<description>TVS DIODE 5.5VWM 8.5VC SOT143</description>
<gates>
<gate name="G$1" symbol="SP0503BAHTG"/>
</gates>
<devices>
<device name="" package="SOT143">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value=" SP050xBA Series 8 V 30 pF Uni-Directional SMT TVS Avalanche Diode Array SOT-143 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="F2715CT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/littelfuse-inc/SP0503BAHTG/F2715CT-ND/1154322?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Littelfuse Inc."/>
<attribute name="MP" value="SP0503BAHTG"/>
<attribute name="PACKAGE" value="SOT-143 Littelfuse"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-2P-1.27MM" prefix="X">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV-1"/>
<gate name="-2" symbol="M-1"/>
</gates>
<devices>
<device name="047" package="53047-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="OC_NEWARK" value="57H4701"/>
</technology>
</technologies>
</device>
<device name="048" package="53048-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53048-0210"/>
<attribute name="OC_FARNELL" value="1012259"/>
<attribute name="OC_NEWARK" value="57H4718"/>
</technology>
</technologies>
</device>
<device name="261" package="53261-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1125373"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="398" package="53398-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSAMD21" prefix="U">
<description>SAMD21E Series 256 KB Flash 32 KB SRAM 48 MHz 32-Bit Microcontroller - QFN-32</description>
<gates>
<gate name="G$1" symbol="ATSAMD21E18A-MU"/>
</gates>
<devices>
<device name="E*-MU" package="QFN50P500X500X100-33N">
<connects>
<connect gate="G$1" pin="!RESET" pad="26"/>
<connect gate="G$1" pin="EP" pad="33"/>
<connect gate="G$1" pin="GND" pad="10 28"/>
<connect gate="G$1" pin="PA00" pad="1"/>
<connect gate="G$1" pin="PA01" pad="2"/>
<connect gate="G$1" pin="PA02" pad="3"/>
<connect gate="G$1" pin="PA03" pad="4"/>
<connect gate="G$1" pin="PA04" pad="5"/>
<connect gate="G$1" pin="PA05" pad="6"/>
<connect gate="G$1" pin="PA06" pad="7"/>
<connect gate="G$1" pin="PA07" pad="8"/>
<connect gate="G$1" pin="PA08" pad="11"/>
<connect gate="G$1" pin="PA09" pad="12"/>
<connect gate="G$1" pin="PA10" pad="13"/>
<connect gate="G$1" pin="PA11" pad="14"/>
<connect gate="G$1" pin="PA14" pad="15"/>
<connect gate="G$1" pin="PA15" pad="16"/>
<connect gate="G$1" pin="PA16" pad="17"/>
<connect gate="G$1" pin="PA17" pad="18"/>
<connect gate="G$1" pin="PA18" pad="19"/>
<connect gate="G$1" pin="PA19" pad="20"/>
<connect gate="G$1" pin="PA22" pad="21"/>
<connect gate="G$1" pin="PA23" pad="22"/>
<connect gate="G$1" pin="PA24" pad="23"/>
<connect gate="G$1" pin="PA25" pad="24"/>
<connect gate="G$1" pin="PA27" pad="25"/>
<connect gate="G$1" pin="PA28" pad="27"/>
<connect gate="G$1" pin="PA30" pad="31"/>
<connect gate="G$1" pin="PA31" pad="32"/>
<connect gate="G$1" pin="VDDANA" pad="9"/>
<connect gate="G$1" pin="VDDCORE" pad="29"/>
<connect gate="G$1" pin="VDDIN" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" SAMD21E Series 256 KB Flash 32 KB SRAM 48 MHz 32-Bit Microcontroller - QFN-32 "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="ATSAMD21E18A-MU"/>
<attribute name="PACKAGE" value="QFN-32 Microchip"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICSP_HEADER" prefix="J">
<gates>
<gate name="G$1" symbol="ICSP"/>
</gates>
<devices>
<device name="ICSP-2MM" package="ICSP_3X2_2MM_STRAIGHT">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="MISO" pad="5"/>
<connect gate="G$1" pin="MOSI" pad="3"/>
<connect gate="G$1" pin="RST" pad="1"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ICSP-2.54MM" package="ICSP_3X2_2.54_STRAIGHT">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="3"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ICSP_2.54MM_RIGHT" package="ICSP_2X3_2.54_RIGHT">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MISO" pad="6"/>
<connect gate="G$1" pin="MOSI" pad="2"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING_2X1.5" package="ICSP_3X2_2X1.5_SPRING_CONTACTS">
<connects>
<connect gate="G$1" pin="GND" pad="2 P$2"/>
<connect gate="G$1" pin="MISO" pad="5 P$5"/>
<connect gate="G$1" pin="MOSI" pad="3 P$3"/>
<connect gate="G$1" pin="RST" pad="1 P$1"/>
<connect gate="G$1" pin="SCK" pad="4 P$4"/>
<connect gate="G$1" pin="VCC" pad="6 P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING_3.48X1.1" package="ICSP_3X2_3.48X1.1_SPRING_CONTACTS">
<connects>
<connect gate="G$1" pin="GND" pad="1 P$1"/>
<connect gate="G$1" pin="MISO" pad="6 P$6"/>
<connect gate="G$1" pin="MOSI" pad="4 P$4"/>
<connect gate="G$1" pin="RST" pad="2 P$2" route="any"/>
<connect gate="G$1" pin="SCK" pad="3 P$3"/>
<connect gate="G$1" pin="VCC" pad="5 P$5" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2PC4081-NPN">
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SC70">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET_ARRAY_EMK34">
<gates>
<gate name="G$1" symbol="LEVEL_SHIFT_NCH_MOSFET"/>
<gate name="G$2" symbol="LEVEL_SHIFT_NCH_MOSFET"/>
</gates>
<devices>
<device name="" package="SOT-563">
<connects>
<connect gate="G$1" pin="D" pad="P$6"/>
<connect gate="G$1" pin="G" pad="P$2"/>
<connect gate="G$1" pin="S" pad="P$1"/>
<connect gate="G$2" pin="D" pad="P$3"/>
<connect gate="G$2" pin="G" pad="P$5"/>
<connect gate="G$2" pin="S" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-SWITCH_SMD-BUTTON(2P-3.0X2.5X1.2+0.4MM)" prefix="SW" uservalue="yes">
<description>311020047</description>
<gates>
<gate name="G$1" symbol="SEEED-SWITCH_BUTTON-2P"/>
</gates>
<devices>
<device name="SW2-2.6-3X2.5X1.2" package="SEEED-SWITCH_SW2-2.6-3.0X2.5X1.2+0.4MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SW2-2.6-3X2.5X1.2_DETAILED_MODEL" package="SEEED-SWITCH_SW2-2.6-3.0X2.5X1.2+0.4MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA48/88/168/328PB" prefix="U">
<description>AVR 32KBytes Flash, 1KBytes EEPROM, 2KBytes RAM, w - 20MHZ, QFN/MFL, IND TEMP, GREEN 5 V/ DFN/QFN (M)</description>
<gates>
<gate name="A" symbol="ATMEGA328PB-MU"/>
<gate name="B" symbol="ATMEGA328PB-MU_PWR"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X90-33N">
<connects>
<connect gate="A" pin="AREF" pad="20"/>
<connect gate="A" pin="PB0/ICP1/CLKO/PTCXY" pad="12"/>
<connect gate="A" pin="PB1/OC1A/PTCXY" pad="13"/>
<connect gate="A" pin="PB2/!SS0!/OC1B/PTCXY" pad="14"/>
<connect gate="A" pin="PB3/MOSI0/TXD1/OC2A/PTCXY" pad="15"/>
<connect gate="A" pin="PB4/MISO0/RXD1/PTCXY" pad="16"/>
<connect gate="A" pin="PB5/PTCXY/XCK1/SCK0" pad="17"/>
<connect gate="A" pin="PB6/XTAL1/TOSC1" pad="7"/>
<connect gate="A" pin="PB7/XTAL2/TOSC2" pad="8"/>
<connect gate="A" pin="PC0/ADC0/PTCY/MISO1" pad="23"/>
<connect gate="A" pin="PC1/ADC1/PTCY/SCK1" pad="24"/>
<connect gate="A" pin="PC2/ADC2/PTCY" pad="25"/>
<connect gate="A" pin="PC3/ADC3/PTCY" pad="26"/>
<connect gate="A" pin="PC4/ADC4/PTCY/SDA0" pad="27"/>
<connect gate="A" pin="PC5/ADC5/PTCY/SCL0" pad="28"/>
<connect gate="A" pin="PC6/!RESET!" pad="29"/>
<connect gate="A" pin="PD0/PTCXY/OC3A/RXD0" pad="30"/>
<connect gate="A" pin="PD1/PTCXY/OC4A/TXD0" pad="31"/>
<connect gate="A" pin="PD2/PTCXY/INT0/OC3B/OC4B" pad="32"/>
<connect gate="A" pin="PD3/OC2B/INT1/PTCXY" pad="1"/>
<connect gate="A" pin="PD4/XCK0/T0/PTCXY" pad="2"/>
<connect gate="A" pin="PD5/OC0B/T1/PTCXY" pad="9"/>
<connect gate="A" pin="PD6/OC0A/PTCXY/AIN0" pad="10"/>
<connect gate="A" pin="PD7/PTCXY/AIN1" pad="11"/>
<connect gate="A" pin="PE0/SDA1/ICP4/ACO/PTCXY" pad="3"/>
<connect gate="A" pin="PE1/SCL1/T4/PTCXY" pad="6"/>
<connect gate="A" pin="PE2/ADC6/PTCY/ICP3/!SS1!" pad="19"/>
<connect gate="A" pin="PE3/ADC7/PTCY/T3/MOSI1" pad="22"/>
<connect gate="B" pin="AVCC" pad="18"/>
<connect gate="B" pin="GND0" pad="5"/>
<connect gate="B" pin="GND1" pad="21"/>
<connect gate="B" pin="PAD" pad="33"/>
<connect gate="B" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" AVR 32KBytes Flash, 1KBytes EEPROM, 2KBytes RAM, w - 20MHZ, QFN/MFL, IND TEMP, GREEN 5 V/ DFN/QFN _M_ "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="ATMEGA328PB-MU"/>
<attribute name="PACKAGE" value="VFQFN-32 Microchip"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FFC-40P-0.5S" prefix="X">
<description>&lt;b&gt;0.5mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
<gates>
<gate name="-1" symbol="PINV"/>
<gate name="-2" symbol="PIN"/>
<gate name="-3" symbol="PIN"/>
<gate name="-4" symbol="PIN"/>
<gate name="-5" symbol="PIN"/>
<gate name="-6" symbol="PIN"/>
<gate name="-7" symbol="PIN"/>
<gate name="-8" symbol="PIN"/>
<gate name="-9" symbol="PIN"/>
<gate name="-10" symbol="PIN"/>
<gate name="-11" symbol="PIN"/>
<gate name="-12" symbol="PIN"/>
<gate name="-13" symbol="PIN"/>
<gate name="-14" symbol="PIN"/>
<gate name="-15" symbol="PIN"/>
<gate name="-16" symbol="PIN"/>
<gate name="-17" symbol="PIN"/>
<gate name="-18" symbol="PIN"/>
<gate name="-19" symbol="PIN"/>
<gate name="-20" symbol="PIN"/>
<gate name="-21" symbol="PIN"/>
<gate name="-22" symbol="PIN"/>
<gate name="-23" symbol="PIN"/>
<gate name="-24" symbol="PIN"/>
<gate name="-25" symbol="PIN"/>
<gate name="-26" symbol="PIN"/>
<gate name="-27" symbol="PIN"/>
<gate name="-28" symbol="PIN"/>
<gate name="-29" symbol="PIN"/>
<gate name="-30" symbol="PIN"/>
<gate name="-31" symbol="PIN"/>
<gate name="-32" symbol="PIN"/>
<gate name="-33" symbol="PIN"/>
<gate name="-34" symbol="PIN"/>
<gate name="-35" symbol="PIN"/>
<gate name="-36" symbol="PIN"/>
<gate name="-37" symbol="PIN"/>
<gate name="-38" symbol="PIN"/>
<gate name="-39" symbol="PIN"/>
<gate name="-40" symbol="PIN"/>
</gates>
<devices>
<device name="H" package="FH12-40S-0.5SH">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-10" pin="1" pad="10"/>
<connect gate="-11" pin="1" pad="11"/>
<connect gate="-12" pin="1" pad="12"/>
<connect gate="-13" pin="1" pad="13"/>
<connect gate="-14" pin="1" pad="14"/>
<connect gate="-15" pin="1" pad="15"/>
<connect gate="-16" pin="1" pad="16"/>
<connect gate="-17" pin="1" pad="17"/>
<connect gate="-18" pin="1" pad="18"/>
<connect gate="-19" pin="1" pad="19"/>
<connect gate="-2" pin="1" pad="2"/>
<connect gate="-20" pin="1" pad="20"/>
<connect gate="-21" pin="1" pad="21"/>
<connect gate="-22" pin="1" pad="22"/>
<connect gate="-23" pin="1" pad="23"/>
<connect gate="-24" pin="1" pad="24"/>
<connect gate="-25" pin="1" pad="25"/>
<connect gate="-26" pin="1" pad="26"/>
<connect gate="-27" pin="1" pad="27"/>
<connect gate="-28" pin="1" pad="28"/>
<connect gate="-29" pin="1" pad="29"/>
<connect gate="-3" pin="1" pad="3"/>
<connect gate="-30" pin="1" pad="30"/>
<connect gate="-31" pin="1" pad="31"/>
<connect gate="-32" pin="1" pad="32"/>
<connect gate="-33" pin="1" pad="33"/>
<connect gate="-34" pin="1" pad="34"/>
<connect gate="-35" pin="1" pad="35"/>
<connect gate="-36" pin="1" pad="36"/>
<connect gate="-37" pin="1" pad="37"/>
<connect gate="-38" pin="1" pad="38"/>
<connect gate="-39" pin="1" pad="39"/>
<connect gate="-4" pin="1" pad="4"/>
<connect gate="-40" pin="1" pad="40"/>
<connect gate="-5" pin="1" pad="5"/>
<connect gate="-6" pin="1" pad="6"/>
<connect gate="-7" pin="1" pad="7"/>
<connect gate="-8" pin="1" pad="8"/>
<connect gate="-9" pin="1" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="FH12-40S-0.5SH(55)"/>
<attribute name="OC_FARNELL" value="1324556"/>
<attribute name="OC_NEWARK" value="34M6178"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSAM4N8">
<description>http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en590799</description>
<gates>
<gate name="G$1" symbol="ATSAM4N8AA-MU_GPIO"/>
<gate name="G$2" symbol="ATSAM4N8AA-MU_PWR"/>
</gates>
<devices>
<device name="48-QFN" package="QFN50P700X700X90-49N">
<connects>
<connect gate="G$1" pin="ADVREFP" pad="1"/>
<connect gate="G$1" pin="ERASE/PB12" pad="42"/>
<connect gate="G$1" pin="JTAGEL" pad="38"/>
<connect gate="G$1" pin="NRST" pad="29"/>
<connect gate="G$1" pin="PA0/PGMEN0" pad="36"/>
<connect gate="G$1" pin="PA1/PGMEN1" pad="35"/>
<connect gate="G$1" pin="PA10/PGMM2" pad="21"/>
<connect gate="G$1" pin="PA11/PGMM3" pad="20"/>
<connect gate="G$1" pin="PA12/PGMD0" pad="19"/>
<connect gate="G$1" pin="PA13/PGMD1" pad="17"/>
<connect gate="G$1" pin="PA14/PGMD2" pad="16"/>
<connect gate="G$1" pin="PA15/PGMD3" pad="15"/>
<connect gate="G$1" pin="PA16/PGMD4" pad="14"/>
<connect gate="G$1" pin="PA17/PGMD5/AD0" pad="9"/>
<connect gate="G$1" pin="PA18/PGMD6/AD1" pad="10"/>
<connect gate="G$1" pin="PA19/PGMD7/AD2" pad="11"/>
<connect gate="G$1" pin="PA2/PGMEN2" pad="32"/>
<connect gate="G$1" pin="PA20/AD3" pad="12"/>
<connect gate="G$1" pin="PA3" pad="31"/>
<connect gate="G$1" pin="PA4/PGMNCMD" pad="28"/>
<connect gate="G$1" pin="PA5/PGMRDY" pad="27"/>
<connect gate="G$1" pin="PA6/PGMNOE" pad="26"/>
<connect gate="G$1" pin="PA7/XIN32/PGMNVALID" pad="24"/>
<connect gate="G$1" pin="PA8/XOUT32/PGMM0" pad="23"/>
<connect gate="G$1" pin="PA9/PGMM1" pad="22"/>
<connect gate="G$1" pin="PB0/AD4" pad="3"/>
<connect gate="G$1" pin="PB1/AD5" pad="4"/>
<connect gate="G$1" pin="PB10" pad="43"/>
<connect gate="G$1" pin="PB11" pad="44"/>
<connect gate="G$1" pin="PB2/AD6" pad="5"/>
<connect gate="G$1" pin="PB3/AD7" pad="6"/>
<connect gate="G$1" pin="PB5/TDO/TRACESWO" pad="37"/>
<connect gate="G$1" pin="PB6/TMS/SWDIO" pad="39"/>
<connect gate="G$1" pin="PB7/TCK/SWCLK" pad="40"/>
<connect gate="G$1" pin="TDI/PB4" pad="25"/>
<connect gate="G$1" pin="TST" pad="30"/>
<connect gate="G$1" pin="XIN/PB9/GMCK" pad="46"/>
<connect gate="G$1" pin="XOUT/PB8" pad="45"/>
<connect gate="G$2" pin="GND0" pad="2"/>
<connect gate="G$2" pin="GND1" pad="34"/>
<connect gate="G$2" pin="PAD" pad="0"/>
<connect gate="G$2" pin="VDDCORE0" pad="18"/>
<connect gate="G$2" pin="VDDCORE1" pad="41"/>
<connect gate="G$2" pin="VDDIN" pad="7"/>
<connect gate="G$2" pin="VDDIO0" pad="13"/>
<connect gate="G$2" pin="VDDIO1" pad="33"/>
<connect gate="G$2" pin="VDDIO2" pad="47"/>
<connect gate="G$2" pin="VDDOUT" pad="8"/>
<connect gate="G$2" pin="VDDPLL" pad="48"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSAM3S4">
<description>http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-6500-32-bit-Cortex-M3-Microcontroller-SAM3S4-SAM3S2-SAM3S1_Datasheet.pdf</description>
<gates>
<gate name="G$1" symbol="ATSAM3S4AA-MU_GPIO"/>
<gate name="G$2" symbol="ATSAM4N8AA-MU_PWR"/>
</gates>
<devices>
<device name="" package="QFN50P700X700X90-49N">
<connects>
<connect gate="G$1" pin="ADVREFP" pad="1"/>
<connect gate="G$1" pin="ERASE/PB12" pad="42"/>
<connect gate="G$1" pin="JTAGEL" pad="38"/>
<connect gate="G$1" pin="NRST" pad="29"/>
<connect gate="G$1" pin="PA0/PGMEN0" pad="36"/>
<connect gate="G$1" pin="PA1/PGMEN1" pad="35"/>
<connect gate="G$1" pin="PA10/PGMM2" pad="21"/>
<connect gate="G$1" pin="PA11/PGMM3" pad="20"/>
<connect gate="G$1" pin="PA12/PGMD0" pad="19"/>
<connect gate="G$1" pin="PA13/PGMD1" pad="17"/>
<connect gate="G$1" pin="PA14/PGMD2" pad="16"/>
<connect gate="G$1" pin="PA15/PGMD3" pad="15"/>
<connect gate="G$1" pin="PA16/PGMD4" pad="14"/>
<connect gate="G$1" pin="PA17/PGMD5/AD0" pad="9"/>
<connect gate="G$1" pin="PA18/PGMD6/AD1" pad="10"/>
<connect gate="G$1" pin="PA19/PGMD7/AD2" pad="11"/>
<connect gate="G$1" pin="PA2/PGMEN2" pad="32"/>
<connect gate="G$1" pin="PA20/AD3" pad="12"/>
<connect gate="G$1" pin="PA3" pad="31"/>
<connect gate="G$1" pin="PA4/PGMNCMD" pad="28"/>
<connect gate="G$1" pin="PA5/PGMRDY" pad="27"/>
<connect gate="G$1" pin="PA6/PGMNOE" pad="26"/>
<connect gate="G$1" pin="PA7/XIN32/PGMNVALID" pad="24"/>
<connect gate="G$1" pin="PA8/XOUT32/PGMM0" pad="23"/>
<connect gate="G$1" pin="PA9/PGMM1" pad="22"/>
<connect gate="G$1" pin="PB0/AD4" pad="3"/>
<connect gate="G$1" pin="PB1/AD5" pad="4"/>
<connect gate="G$1" pin="PB10/DDM" pad="43"/>
<connect gate="G$1" pin="PB11/DDP" pad="44"/>
<connect gate="G$1" pin="PB2/AD6" pad="5"/>
<connect gate="G$1" pin="PB3/AD7" pad="6"/>
<connect gate="G$1" pin="PB5/TDO/TRACESWO" pad="37"/>
<connect gate="G$1" pin="PB6/TMS/SWDIO" pad="39"/>
<connect gate="G$1" pin="PB7/TCK/SWCLK" pad="40"/>
<connect gate="G$1" pin="TDI/PB4" pad="25"/>
<connect gate="G$1" pin="TST" pad="30"/>
<connect gate="G$1" pin="XIN/PB9/GMCK" pad="46"/>
<connect gate="G$1" pin="XOUT/PB8" pad="45"/>
<connect gate="G$2" pin="GND0" pad="2"/>
<connect gate="G$2" pin="GND1" pad="34"/>
<connect gate="G$2" pin="PAD" pad="0"/>
<connect gate="G$2" pin="VDDCORE0" pad="18"/>
<connect gate="G$2" pin="VDDCORE1" pad="41"/>
<connect gate="G$2" pin="VDDIN" pad="7"/>
<connect gate="G$2" pin="VDDIO0" pad="13"/>
<connect gate="G$2" pin="VDDIO1" pad="33"/>
<connect gate="G$2" pin="VDDIO2" pad="47"/>
<connect gate="G$2" pin="VDDOUT" pad="8"/>
<connect gate="G$2" pin="VDDPLL" pad="48"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R1003F" prefix="L" uservalue="yes">
<description>Gegentakt-Entstördrossel
differential mode choke</description>
<gates>
<gate name="G$1" symbol="SINGLE"/>
</gates>
<devices>
<device name="-SMD" package="SMD">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="B5" package="B5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S11" package="S11-10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="B6" package="B6">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-SWITCH_DIP-TOGGLE-SWITCH-2CH-(2X3P-2.54)" prefix="SW" uservalue="yes">
<description>311010004</description>
<gates>
<gate name="G$1" symbol="SEEED-SWITCH_SWITCH-2CH-6P"/>
</gates>
<devices>
<device name="DPDT_254_6P_UPDATE" package="SEEED-SWITCH_SW6-2.54-9.0X3.5X3.2+2.0MM">
<connects>
<connect gate="G$1" pin="CH1A" pad="CH1A"/>
<connect gate="G$1" pin="CH1B" pad="CH1B"/>
<connect gate="G$1" pin="CH2A" pad="CH2A"/>
<connect gate="G$1" pin="CH2B" pad="CH2B"/>
<connect gate="G$1" pin="COM1" pad="COM1"/>
<connect gate="G$1" pin="COM2" pad="COM2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2902" prefix="U">
<description>&lt;b&gt;Low power quad operational amplifier&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00000533.pdf"&gt; Data sgeet &lt;/a&gt;</description>
<gates>
<gate name="A" symbol="OPAMP-1"/>
<gate name="B" symbol="OPAMP-1"/>
<gate name="C" symbol="OPAMP-1"/>
<gate name="D" symbol="OPAMP-1"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT" package="SSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QT" package="QFN16">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="16"/>
<connect gate="A" pin="OUT" pad="15"/>
<connect gate="B" pin="+IN" pad="4"/>
<connect gate="B" pin="-IN" pad="5"/>
<connect gate="B" pin="OUT" pad="6"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="7"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="2"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22-23-2021" prefix="X">
<description>.100" (2.54mm) Center Header - 2 Pin</description>
<gates>
<gate name="-1" symbol="MV-3"/>
<gate name="-2" symbol="M-3"/>
</gates>
<devices>
<device name="" package="22-23-2021">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FUSE_0402" prefix="F">
<description>https://www.digikey.com/product-detail/en/ERB-RD0R50X/P15122CT-ND/2796798/?itemSeq=282912571</description>
<gates>
<gate name="G$1" symbol="FUSE"/>
</gates>
<devices>
<device name="FUSE_0402" package="FUSE_0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
&lt;u&gt;OSRAM&lt;/u&gt;:&lt;br&gt;

- &lt;u&gt;CHIPLED&lt;/u&gt;&lt;br&gt;
LG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971
LH N974, LH R974&lt;br&gt;
LS Q976, LO Q976, LY Q976&lt;br&gt;
LO Q996&lt;br&gt;

- &lt;u&gt;Hyper CHIPLED&lt;/u&gt;&lt;br&gt;
LW Q18S&lt;br&gt;
LB Q993, LB Q99A, LB R99A&lt;br&gt;

- &lt;u&gt;SideLED&lt;/u&gt;&lt;br&gt;
LS A670, LO A670, LY A670, LG A670, LP A670&lt;br&gt;
LB A673, LV A673, LT A673, LW A673&lt;br&gt;
LH A674&lt;br&gt;
LY A675&lt;br&gt;
LS A676, LA A676, LO A676, LY A676, LW A676&lt;br&gt;
LS A679, LY A679, LG A679&lt;br&gt;

-  &lt;u&gt;Hyper Micro SIDELED®&lt;/u&gt;&lt;br&gt;
LS Y876, LA Y876, LO Y876, LY Y876&lt;br&gt;
LT Y87S&lt;br&gt;

- &lt;u&gt;SmartLED&lt;/u&gt;&lt;br&gt;
LW L88C, LW L88S&lt;br&gt;
LB L89C, LB L89S, LG L890&lt;br&gt;
LS L89K, LO L89K, LY L89K&lt;br&gt;
LS L896, LA L896, LO L896, LY L896&lt;br&gt;

- &lt;u&gt;TOPLED&lt;/u&gt;&lt;br&gt;
LS T670, LO T670, LY T670, LG T670, LP T670&lt;br&gt;
LSG T670, LSP T670, LSY T670, LOP T670, LYG T670&lt;br&gt;
LG T671, LOG T671, LSG T671&lt;br&gt;
LB T673, LV T673, LT T673, LW T673&lt;br&gt;
LH T674&lt;br&gt;
LS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676&lt;br&gt;
LB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C&lt;br&gt;
LW T67C&lt;br&gt;
LS T679, LY T679, LG T679&lt;br&gt;
LS T770, LO T770, LY T770, LG T770, LP T770&lt;br&gt;
LB T773, LV T773, LT T773, LW T773&lt;br&gt;
LH T774&lt;br&gt;
LS E675, LA E675, LY E675, LS T675&lt;br&gt;
LS T776, LA T776, LO T776, LY T776, LB T776&lt;br&gt;
LHGB T686&lt;br&gt;
LT T68C, LB T68C&lt;br&gt;

- &lt;u&gt;Hyper Mini TOPLED®&lt;/u&gt;&lt;br&gt;
LB M676&lt;br&gt;

- &lt;u&gt;Mini TOPLED Santana®&lt;/u&gt;&lt;br&gt;
LG M470&lt;br&gt;
LS M47K, LO M47K, LY M47K
&lt;p&gt;
Source: http://www.osram.convergy.de&lt;p&gt;

&lt;u&gt;LUXEON:&lt;/u&gt;&lt;br&gt;
- &lt;u&gt;LUMILED®&lt;/u&gt;&lt;br&gt;
LXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00&lt;br&gt;
LXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00&lt;br&gt;
LXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00&lt;br&gt;
LXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00&lt;br&gt;
LXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00&lt;br&gt;
LXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00&lt;br&gt;
LXK2-PH12-R00, LXK2-PH12-S00&lt;br&gt;
LXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00
&lt;p&gt;
Source: www.luxeon.com&lt;p&gt;

&lt;u&gt;KINGBRIGHT:&lt;/U&gt;&lt;p&gt;
KA-3528ASYC&lt;br&gt;
Source: www.kingbright.com</description>
<gates>
<gate name="G$1" symbol="LED-1"/>
</gates>
<devices>
<device name="SMT1206" package="1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LD260" package="LD260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR2X5" package="LED2X5">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LSU260" package="LSU260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZR181" package="LZR181">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B152" package="Q62902-B152">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B153" package="Q62902-B153">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B155" package="Q62902-B155">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B156" package="Q62902-B156">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH480" package="SFH480">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH482" package="SFH482">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR5.7X3.2" package="U57X32">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRL80A" package="IRL80A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2" package="P-LCC-2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-TOP" package="OSRAM-MINI-TOP-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIDELED" package="OSRAM-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMART-LED" package="SMART-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2-BACK" package="P-LCC-2-TOPLED-RG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MICRO-SIDELED" package="MICRO-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-4" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0603" package="CHIP-LED0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0805" package="CHIP-LED0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOPLED-SANTANA" package="MINI-TOPLED-SANTANA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0805" package="CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_1206" package="CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED-0603-TTW" package="CHIPLED-0603-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SMARTLED-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED+" package="LUMILED+">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED" package="LUMILED">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KA-3528ASYC" package="KA-3528ASYC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML0805" package="SML0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML1206" package="SML1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML0603" package="SML0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-3P-1.25MM" prefix="X">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV-2"/>
<gate name="-2" symbol="M-2"/>
<gate name="-3" symbol="M-2"/>
</gates>
<devices>
<device name="047" package="53047-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="530470310"/>
<attribute name="OC_FARNELL" value="9732853"/>
<attribute name="OC_NEWARK" value="14R5412"/>
</technology>
</technologies>
</device>
<device name="048" package="53048-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="WALDOM/MOLEX"/>
<attribute name="MPN" value="53048-0310"/>
<attribute name="OC_FARNELL" value="9732918"/>
<attribute name="OC_NEWARK" value="38C9908"/>
</technology>
</technologies>
</device>
<device name="261" package="53261-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53261-0390"/>
<attribute name="OC_FARNELL" value="1125359"/>
<attribute name="OC_NEWARK" value="57H5006"/>
</technology>
</technologies>
</device>
<device name="398" package="53398-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST-2.54-2X2">
<gates>
<gate name="A" symbol="M"/>
<gate name="B" symbol="M"/>
<gate name="C" symbol="M"/>
<gate name="D" symbol="M"/>
</gates>
<devices>
<device name="JST-DUPONT-2.54-2X2" package="HDRRAR4W64P254_2X2_556X736X556B">
<connects>
<connect gate="A" pin="S" pad="1"/>
<connect gate="B" pin="S" pad="2"/>
<connect gate="C" pin="S" pad="3"/>
<connect gate="D" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HOLES_MOUNT-PAD-ROUND" prefix="H">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt;, round</description>
<gates>
<gate name="G$1" symbol="HOLES_MOUNT-PAD"/>
</gates>
<devices>
<device name="2.8" package="HOLES_2,8-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B2,8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.0" package="HOLES_3,0-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,0"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.2" package="HOLES_3,2-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.3" package="HOLES_3,3-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.6" package="HOLES_3,6-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.1" package="HOLES_4,1-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.3" package="HOLES_4,3-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.5" package="HOLES_4,5-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.0" package="HOLES_5,0-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.5" package="HOLES_5,5-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B5,5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HOLES_2,8-PAD-W-SCREW" package="HOLES_2,8-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B2,8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP6001T-I/OT" prefix="U">
<gates>
<gate name="A" symbol="MCP6001T-I/OT"/>
</gates>
<devices>
<device name="" package="SOT-23-5_MC">
<connects>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP6001TIOT"/>
<attribute name="VENDOR" value="Microchip"/>
</technology>
</technologies>
</device>
<device name="SOT-23-5_MC-M" package="SOT-23-5_MC-M">
<connects>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP6001TIOT"/>
<attribute name="VENDOR" value="Microchip"/>
</technology>
</technologies>
</device>
<device name="SOT-23-5_MC-L" package="SOT-23-5_MC-L">
<connects>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="VIN+" pad="3"/>
<connect gate="A" pin="VIN-" pad="4"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP6001TIOT"/>
<attribute name="VENDOR" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCS08" prefix="LSP">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt; MC S0,8, drill 1.2 mm, distributor Buerklin, 08F130</description>
<gates>
<gate name="G$1" symbol="LSP"/>
</gates>
<devices>
<device name="" package="MCS08">
<connects>
<connect gate="G$1" pin="MP" pad="MP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-LED_SMD-LED-CLEAR-BLUE(0603)" prefix="D" uservalue="yes">
<description>304090045</description>
<gates>
<gate name="G$1" symbol="SEEED-LED_LED-1"/>
</gates>
<devices>
<device name="LED_0603" package="SEEED-LED_LED-0603">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC33X-2-103E" prefix="VR">
<description>Res Cermet POT 10K Ohm 25% 0.1W(1/10W) 1(Elec)/1(Mech)Turn 3mm (3 X 3.65 X 1.85mm) Foot Print SMD T/R</description>
<gates>
<gate name="G$1" symbol="TC33X-2-103E"/>
</gates>
<devices>
<device name="" package="TRIM_TC33X-2-103E">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Res Trimmer 10K Ohm 25% 0.1W_1/10W_ 1_Elec_/1_Mech_Turn _3 X 3.8mm_ Foot Print SMD Embossed T/R "/>
<attribute name="MF" value="Bourns"/>
<attribute name="MP" value="TC33X-2-103E"/>
<attribute name="PACKAGE" value="FakePackage u"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-COM_ANO" prefix="D">
<description>&lt;h3&gt;Everlight Electronics Co Ltd EAST1616RGBB4 0606 RGB LED&lt;/h3&gt;

&lt;p&gt;&lt;li&gt;&lt;b&gt;Color:&lt;/b&gt; RGB&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Lens Transparency: &lt;/b&gt; Clear&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Lens Style/Size:&lt;/b&gt; Rectangle with Flat top, 1.10 x 1.5 mm&lt;/li&gt;
&lt;li&gt;&lt;b&gt;mC Rating&lt;/b&gt;45mcd Red, 35 mcd Green&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Current:&lt;/b&gt; 5mA Red, 5mA Green, 5mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Forward Voltage: &lt;/b&gt; 2V Red, 2V Green&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt; 0606&lt;/li&gt;
&lt;/p&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/12958]”&gt;Electric Imp imp002 Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RGB_COM_ANO"/>
</gates>
<devices>
<device name="0606" package="0606_LED">
<connects>
<connect gate="G$1" pin="ANO" pad="P$2"/>
<connect gate="G$1" pin="BLU" pad="P$4"/>
<connect gate="G$1" pin="GRN" pad="P$3"/>
<connect gate="G$1" pin="RED" pad="P$1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12140"/>
</technology>
</technologies>
</device>
<device name="4PLCC" package="4PLCC">
<connects>
<connect gate="G$1" pin="ANO" pad="P$1"/>
<connect gate="G$1" pin="BLU" pad="P$4"/>
<connect gate="G$1" pin="GRN" pad="P$3"/>
<connect gate="G$1" pin="RED" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_SCHOTTKY_SINGLE" prefix="D">
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="" package="DO-214AC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SFW24R-1STE1LF" prefix="J">
<gates>
<gate name="A" symbol="CON24_1X24_DRB_SFW"/>
</gates>
<devices>
<device name="" package="CON24_1X24_DRB_SFW">
<connects>
<connect gate="A" pin="1010" pad="10"/>
<connect gate="A" pin="11" pad="1"/>
<connect gate="A" pin="1111" pad="11"/>
<connect gate="A" pin="1212" pad="12"/>
<connect gate="A" pin="1313" pad="13"/>
<connect gate="A" pin="1414" pad="14"/>
<connect gate="A" pin="1515" pad="15"/>
<connect gate="A" pin="1616" pad="16"/>
<connect gate="A" pin="1717" pad="17"/>
<connect gate="A" pin="1818" pad="18"/>
<connect gate="A" pin="1919" pad="19"/>
<connect gate="A" pin="2020" pad="20"/>
<connect gate="A" pin="2121" pad="21"/>
<connect gate="A" pin="22" pad="2"/>
<connect gate="A" pin="2222" pad="22"/>
<connect gate="A" pin="2323" pad="23"/>
<connect gate="A" pin="2424" pad="24"/>
<connect gate="A" pin="2525" pad="25"/>
<connect gate="A" pin="2626" pad="26"/>
<connect gate="A" pin="33" pad="3"/>
<connect gate="A" pin="44" pad="4"/>
<connect gate="A" pin="55" pad="5"/>
<connect gate="A" pin="66" pad="6"/>
<connect gate="A" pin="77" pad="7"/>
<connect gate="A" pin="88" pad="8"/>
<connect gate="A" pin="99" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="SFW24R1STE1LF"/>
<attribute name="VENDOR" value="FCI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-GRID-03" prefix="J">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 2.54 mm (0.100") pitch header</description>
<gates>
<gate name="-1" symbol="MV-3"/>
<gate name="-2" symbol="M-3"/>
<gate name="-3" symbol="M-3"/>
</gates>
<devices>
<device name="-70543" package="70543-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-70553" package="70553-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-74099" package="74099-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-15-91" package="15-91-03">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA48/88/168/328PA" prefix="U">
<gates>
<gate name="A" symbol="ATMEGA48PA-MMHR"/>
<gate name="B" symbol="ATMEGA48PA-MMHR_A"/>
</gates>
<devices>
<device name="" package="28M1">
<connects>
<connect gate="A" pin="(PCINT0/CLKO/ICP1)_PB0" pad="10"/>
<connect gate="A" pin="(PCINT1/OC1A)_PB1" pad="11"/>
<connect gate="A" pin="(PCINT19/OC2B/INT1)_PD3" pad="1"/>
<connect gate="A" pin="(PCINT2/SS/OC1B)_PB2" pad="12"/>
<connect gate="A" pin="(PCINT20/XCK/T0)_PD4" pad="2"/>
<connect gate="A" pin="(PCINT21/OC0B/T1)_PD5" pad="7"/>
<connect gate="A" pin="(PCINT22/OC0A/AIN0)_PD6" pad="8"/>
<connect gate="A" pin="(PCINT23/AIN1)_PD7" pad="9"/>
<connect gate="A" pin="(PCINT3/OC2A/MOSI)_PB3" pad="13"/>
<connect gate="A" pin="(PCINT4/MISO)_PB4" pad="14"/>
<connect gate="A" pin="(PCINT6/XTAL1/TOSC1)_PB6" pad="5"/>
<connect gate="A" pin="(PCINT7/XTAL2/TOSC2)_PB7" pad="6"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="AREF" pad="17"/>
<connect gate="A" pin="PB5_(SCK/PCINT5)" pad="15"/>
<connect gate="A" pin="PC0_(ADC0/PCINT8)" pad="19"/>
<connect gate="A" pin="PC1_(ADC1/PCINT9)" pad="20"/>
<connect gate="A" pin="PC2_(ADC2/PCINT10)" pad="21"/>
<connect gate="A" pin="PC3_(ADC3/PCINT11)" pad="22"/>
<connect gate="A" pin="PC4_(ADC4/SDA/PCINT12)" pad="23"/>
<connect gate="A" pin="PC5_(ADC5/SCL/PCINT13)" pad="24"/>
<connect gate="A" pin="PC6_(RESET/PCINT14)" pad="25"/>
<connect gate="A" pin="PD0_(RXD/PCINT16)" pad="26"/>
<connect gate="A" pin="PD1_(TXD/PCINT17)" pad="27"/>
<connect gate="A" pin="PD2_(INT0/PCINT18)" pad="28"/>
<connect gate="B" pin="AVCC" pad="16"/>
<connect gate="B" pin="GND" pad="18"/>
<connect gate="B" pin="GND_2" pad="4"/>
<connect gate="B" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA48PAMMHR"/>
<attribute name="VENDOR" value="Atmel"/>
</technology>
</technologies>
</device>
<device name="28M1-M" package="28M1-M">
<connects>
<connect gate="A" pin="(PCINT0/CLKO/ICP1)_PB0" pad="10"/>
<connect gate="A" pin="(PCINT1/OC1A)_PB1" pad="11"/>
<connect gate="A" pin="(PCINT19/OC2B/INT1)_PD3" pad="1"/>
<connect gate="A" pin="(PCINT2/SS/OC1B)_PB2" pad="12"/>
<connect gate="A" pin="(PCINT20/XCK/T0)_PD4" pad="2"/>
<connect gate="A" pin="(PCINT21/OC0B/T1)_PD5" pad="7"/>
<connect gate="A" pin="(PCINT22/OC0A/AIN0)_PD6" pad="8"/>
<connect gate="A" pin="(PCINT23/AIN1)_PD7" pad="9"/>
<connect gate="A" pin="(PCINT3/OC2A/MOSI)_PB3" pad="13"/>
<connect gate="A" pin="(PCINT4/MISO)_PB4" pad="14"/>
<connect gate="A" pin="(PCINT6/XTAL1/TOSC1)_PB6" pad="5"/>
<connect gate="A" pin="(PCINT7/XTAL2/TOSC2)_PB7" pad="6"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="AREF" pad="17"/>
<connect gate="A" pin="PB5_(SCK/PCINT5)" pad="15"/>
<connect gate="A" pin="PC0_(ADC0/PCINT8)" pad="19"/>
<connect gate="A" pin="PC1_(ADC1/PCINT9)" pad="20"/>
<connect gate="A" pin="PC2_(ADC2/PCINT10)" pad="21"/>
<connect gate="A" pin="PC3_(ADC3/PCINT11)" pad="22"/>
<connect gate="A" pin="PC4_(ADC4/SDA/PCINT12)" pad="23"/>
<connect gate="A" pin="PC5_(ADC5/SCL/PCINT13)" pad="24"/>
<connect gate="A" pin="PC6_(RESET/PCINT14)" pad="25"/>
<connect gate="A" pin="PD0_(RXD/PCINT16)" pad="26"/>
<connect gate="A" pin="PD1_(TXD/PCINT17)" pad="27"/>
<connect gate="A" pin="PD2_(INT0/PCINT18)" pad="28"/>
<connect gate="B" pin="AVCC" pad="16"/>
<connect gate="B" pin="GND" pad="18"/>
<connect gate="B" pin="GND_2" pad="4"/>
<connect gate="B" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA48PAMMHR"/>
<attribute name="VENDOR" value="Atmel"/>
</technology>
</technologies>
</device>
<device name="28M1-L" package="28M1-L">
<connects>
<connect gate="A" pin="(PCINT0/CLKO/ICP1)_PB0" pad="10"/>
<connect gate="A" pin="(PCINT1/OC1A)_PB1" pad="11"/>
<connect gate="A" pin="(PCINT19/OC2B/INT1)_PD3" pad="1"/>
<connect gate="A" pin="(PCINT2/SS/OC1B)_PB2" pad="12"/>
<connect gate="A" pin="(PCINT20/XCK/T0)_PD4" pad="2"/>
<connect gate="A" pin="(PCINT21/OC0B/T1)_PD5" pad="7"/>
<connect gate="A" pin="(PCINT22/OC0A/AIN0)_PD6" pad="8"/>
<connect gate="A" pin="(PCINT23/AIN1)_PD7" pad="9"/>
<connect gate="A" pin="(PCINT3/OC2A/MOSI)_PB3" pad="13"/>
<connect gate="A" pin="(PCINT4/MISO)_PB4" pad="14"/>
<connect gate="A" pin="(PCINT6/XTAL1/TOSC1)_PB6" pad="5"/>
<connect gate="A" pin="(PCINT7/XTAL2/TOSC2)_PB7" pad="6"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="AREF" pad="17"/>
<connect gate="A" pin="PB5_(SCK/PCINT5)" pad="15"/>
<connect gate="A" pin="PC0_(ADC0/PCINT8)" pad="19"/>
<connect gate="A" pin="PC1_(ADC1/PCINT9)" pad="20"/>
<connect gate="A" pin="PC2_(ADC2/PCINT10)" pad="21"/>
<connect gate="A" pin="PC3_(ADC3/PCINT11)" pad="22"/>
<connect gate="A" pin="PC4_(ADC4/SDA/PCINT12)" pad="23"/>
<connect gate="A" pin="PC5_(ADC5/SCL/PCINT13)" pad="24"/>
<connect gate="A" pin="PC6_(RESET/PCINT14)" pad="25"/>
<connect gate="A" pin="PD0_(RXD/PCINT16)" pad="26"/>
<connect gate="A" pin="PD1_(TXD/PCINT17)" pad="27"/>
<connect gate="A" pin="PD2_(INT0/PCINT18)" pad="28"/>
<connect gate="B" pin="AVCC" pad="16"/>
<connect gate="B" pin="GND" pad="18"/>
<connect gate="B" pin="GND_2" pad="4"/>
<connect gate="B" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA48PAMMHR"/>
<attribute name="VENDOR" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_SCHOTTKY_2-ARRAY" prefix="D">
<description>https://media.digikey.com/pdf/Data%20Sheets/Vishay%20Semiconductors/V8KM60DU.pdf</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
<gate name="G$2" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="" package="8-POWERTDFN">
<connects>
<connect gate="G$1" pin="A" pad="P$1 P$2"/>
<connect gate="G$1" pin="C" pad="F1 F2-1 P$7 P$8"/>
<connect gate="G$2" pin="A" pad="P$3 P$4"/>
<connect gate="G$2" pin="C" pad="F2 F2-2 P$5 P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-PYR0BALL">
<gates>
<gate name="G$1" symbol="LOGO-PYR0BALL"/>
</gates>
<devices>
<device name="SILKSCREEN-15MM" package="LOGO-PYR0BALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EMBOSS-KEEPOUT-20MM" package="LOGO-PYR0BALL-IMPRESSION">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EMBOSS-KEEPOUT-15MM" package="LOGO-PYR0BALL-EMBOSS-15MM">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EMBOSS-KEEPOUT-35MM" package="LOGO-PYR0BALL-EMBOSS-35MM">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SILKSCREEN-20MM" package="LOGO-PYR0BALL-SS-20MM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_TVS_ARRAY_CM1293A" prefix="D">
<description>https://www.onsemi.com/pub/Collateral/CM1293A-D.PDF</description>
<gates>
<gate name="G$1" symbol="TVS_DIODE_PRIMARY"/>
<gate name="G$2" symbol="TVS_DIODE_CHANNEL"/>
<gate name="G$3" symbol="TVS_DIODE_CHANNEL"/>
<gate name="G$4" symbol="TVS_DIODE_CHANNEL"/>
</gates>
<devices>
<device name="" package="SC-74-6">
<connects>
<connect gate="G$1" pin="CH$1" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
<connect gate="G$2" pin="CH$1" pad="3"/>
<connect gate="G$3" pin="CH$1" pad="4"/>
<connect gate="G$4" pin="CH$1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1N4148" prefix="D">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
high speed (Philips)</description>
<gates>
<gate name="G$1" symbol="D"/>
</gates>
<devices>
<device name="DO35-10" package="DO35-10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO35-7" package="DO35-7">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DFN-1006-2" package="DIOC1006X70">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358PWR" prefix="U">
<gates>
<gate name="A" symbol="OPAMP+GN"/>
<gate name="B" symbol="OPAMP"/>
</gates>
<devices>
<device name="" package="PW8">
<connects>
<connect gate="A" pin="1IN+" pad="3"/>
<connect gate="A" pin="1IN-" pad="2"/>
<connect gate="A" pin="1OUT" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="B" pin="2IN+" pad="5"/>
<connect gate="B" pin="2IN-" pad="6"/>
<connect gate="B" pin="2OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="LM358PWR"/>
<attribute name="VENDOR" value="Vendor"/>
</technology>
</technologies>
</device>
<device name="PW8-M" package="PW8-M">
<connects>
<connect gate="A" pin="1IN+" pad="3"/>
<connect gate="A" pin="1IN-" pad="2"/>
<connect gate="A" pin="1OUT" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="B" pin="2IN+" pad="5"/>
<connect gate="B" pin="2IN-" pad="6"/>
<connect gate="B" pin="2OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="LM358PWR"/>
<attribute name="VENDOR" value="Vendor"/>
</technology>
</technologies>
</device>
<device name="PW8-L" package="PW8-L">
<connects>
<connect gate="A" pin="1IN+" pad="3"/>
<connect gate="A" pin="1IN-" pad="2"/>
<connect gate="A" pin="1OUT" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="B" pin="2IN+" pad="5"/>
<connect gate="B" pin="2IN-" pad="6"/>
<connect gate="B" pin="2OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MANUFACTURER_PART_NUMBER" value="LM358PWR"/>
<attribute name="VENDOR" value="Vendor"/>
</technology>
</technologies>
</device>
<device name="DFN-8" package="SON50P200X200X60-9N">
<connects>
<connect gate="A" pin="1IN+" pad="3"/>
<connect gate="A" pin="1IN-" pad="2"/>
<connect gate="A" pin="1OUT" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="B" pin="2IN+" pad="5"/>
<connect gate="B" pin="2IN-" pad="6"/>
<connect gate="B" pin="2OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP-ALUMINUM-100UF-16V(D5-H7MM)" prefix="C" uservalue="yes">
<description>302030031</description>
<gates>
<gate name="G$1" symbol="CAP-POLAR"/>
</gates>
<devices>
<device name="LEFT" package="ALU-C-D5.3MM_LEFT">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="KS 100uF/16V"/>
<attribute name="VALUE" value="100uf"/>
</technology>
</technologies>
</device>
<device name="LEFT_SS" package="CAPPRD254W65D650H1250B">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RIGHT" package="ALU-C-D5.3MM_RIGHT">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PP-STANDALONE-HEADER">
<gates>
<gate name="G$1" symbol="PP-STANDALONE-GADJ"/>
<gate name="G$2" symbol="PP-STANDALONE-OUTPUT"/>
<gate name="G$3" symbol="PP-STANDALONE-POWER"/>
<gate name="G$4" symbol="PP-STANDALONE-PWM"/>
<gate name="G$5" symbol="PP-STANDALONE-SENSE"/>
</gates>
<devices>
<device name="" package="PP-STANDALONE-HEADER">
<connects>
<connect gate="G$1" pin="GADG_R0" pad="2"/>
<connect gate="G$1" pin="GADG_R1" pad="3"/>
<connect gate="G$1" pin="GADG_R2" pad="4"/>
<connect gate="G$1" pin="GADG_R3" pad="5"/>
<connect gate="G$2" pin="PT100" pad="6"/>
<connect gate="G$2" pin="Z-TRG" pad="12"/>
<connect gate="G$3" pin="GND" pad="7"/>
<connect gate="G$3" pin="VCC" pad="1"/>
<connect gate="G$4" pin="COMP_PWM" pad="8"/>
<connect gate="G$4" pin="FOL_PWM" pad="9"/>
<connect gate="G$5" pin="COMP_S" pad="10"/>
<connect gate="G$5" pin="FOL_S" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MTA03-156" prefix="J" uservalue="yes">
<description>&lt;b&gt;AMP connector&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MTA-03"/>
</gates>
<devices>
<device name="" package="1X3MTA">
<connects>
<connect gate="G$2" pin="1" pad="1"/>
<connect gate="G$2" pin="2" pad="2"/>
<connect gate="G$2" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="POPULARITY" value="0"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY84A-MMH" prefix="U">
<description>MCU, 8BIT, AVR, 8K FLASH,</description>
<gates>
<gate name="A" symbol="ATTINY84A-MMH"/>
</gates>
<devices>
<device name="" package="QFN45P300X300X85-21N">
<connects>
<connect gate="A" pin="DNC" pad="10"/>
<connect gate="A" pin="DNC_2" pad="17"/>
<connect gate="A" pin="DNC_3" pad="18"/>
<connect gate="A" pin="DNC_4" pad="6"/>
<connect gate="A" pin="DNC_5" pad="19"/>
<connect gate="A" pin="DNC_6" pad="7"/>
<connect gate="A" pin="GND" pad="21"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="PA0" pad="5"/>
<connect gate="A" pin="PA1" pad="4"/>
<connect gate="A" pin="PA2" pad="3"/>
<connect gate="A" pin="PA3" pad="2"/>
<connect gate="A" pin="PA4" pad="1"/>
<connect gate="A" pin="PA5" pad="20"/>
<connect gate="A" pin="PA6" pad="16"/>
<connect gate="A" pin="PA7" pad="15"/>
<connect gate="A" pin="PB0" pad="11"/>
<connect gate="A" pin="PB1" pad="12"/>
<connect gate="A" pin="PB2" pad="14"/>
<connect gate="A" pin="PB3" pad="13"/>
<connect gate="A" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY84A-MMH"/>
<attribute name="OC_FARNELL" value="1972168 "/>
<attribute name="OC_NEWARK" value="68T3788"/>
<attribute name="PACKAGE" value="20-VQFN"/>
<attribute name="SUPPLIER" value="ATMEL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP6232T-E/MS" prefix="U">
<description>IC, OP AMP, 1.8V, DUAL, R-R</description>
<gates>
<gate name="A" symbol="MCP6232T-E/MS"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VINA+" pad="3"/>
<connect gate="A" pin="VINA-" pad="2"/>
<connect gate="A" pin="VINB+" pad="5"/>
<connect gate="A" pin="VINB-" pad="6"/>
<connect gate="A" pin="VOUTA" pad="1"/>
<connect gate="A" pin="VOUTB" pad="7"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" MCP6232 Series 6 V 300 kHz Thru Hole Rail-to-Rail Operational Amplifier - MSOP-8 "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="MCP6232T-E/MS"/>
<attribute name="PACKAGE" value="MSOP-8 Microchip"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TP" prefix="TP">
<description>&lt;b&gt;Test pad&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TP"/>
</gates>
<devices>
<device name="B1,27" package="B1,27">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="B2,54" package="B2,54">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-13" package="P1-13">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-13Y" package="P1-13Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-17" package="P1-17">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-17Y" package="P1-17Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-20" package="P1-20">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-20Y" package="P1-20Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP06R" package="TP06R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP06SQ" package="TP06SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP07R" package="TP07R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP07SQ" package="TP07SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP08R" package="TP08R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP08SQ" package="TP08SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP09R" package="TP09R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP09SQ" package="TP09SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP10R" package="TP10R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP10SQ" package="TP10SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP11R" package="TP11R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP11SQ" package="TP11SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP12SQ" package="TP12SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP12R" package="TP12R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP13R" package="TP13R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP14R" package="TP14R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP15R" package="TP15R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP16R" package="TP16R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP17R" package="TP17R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP18R" package="TP18R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP19R" package="TP19R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP20R" package="TP20R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP13SQ" package="TP13SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP14SQ" package="TP14SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP15SQ" package="TP15SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP16SQ" package="TP16SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP17SQ" package="TP17SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP18SQ" package="TP18SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP19SQ" package="TP19SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP20SQ" package="TP20SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="" package="TP13SQ-HOLE">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING_CONTACT_2X1.5" package="SPRING_CONTACT_2.5X1.5">
<connects>
<connect gate="G$1" pin="TP" pad="TH TP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING_CONTACT_3.5X1.1" package="SPRING_CONTACT_3.48X1.10">
<connects>
<connect gate="G$1" pin="TP" pad="TH TP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-GRID-02" prefix="X">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 2.54 mm (0.100") pitch header</description>
<gates>
<gate name="-2" symbol="M-3"/>
<gate name="-1" symbol="MV-3"/>
</gates>
<devices>
<device name="-70543" package="70543-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-70553" package="70553-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-15-19" package="15-91-02">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-6P-1.25MM" prefix="X">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;&#xD;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV-5"/>
<gate name="-2" symbol="M-5"/>
<gate name="-3" symbol="M-5"/>
<gate name="-4" symbol="M-5"/>
<gate name="-5" symbol="M-5"/>
<gate name="-6" symbol="M-5"/>
</gates>
<devices>
<device name="047" package="53047-06">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53047-0610-C"/>
<attribute name="OC_FARNELL" value="9733078"/>
<attribute name="OC_NEWARK" value="03M2965"/>
</technology>
</technologies>
</device>
<device name="048" package="53048-06">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="WALDOM/MOLEX"/>
<attribute name="MPN" value="53048-0610"/>
<attribute name="OC_FARNELL" value="1012260"/>
<attribute name="OC_NEWARK" value="38C9911"/>
</technology>
</technologies>
</device>
<device name="261" package="53261-06">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1125375"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="398" package="53398-06">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
<connect gate="-6" pin="S" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1125368"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX-4P-1.25MM" prefix="X">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;&#xD;
wire to board 1.25 mm (.049 inch) pitch header</description>
<gates>
<gate name="-1" symbol="MV-4"/>
<gate name="-2" symbol="M-4"/>
<gate name="-3" symbol="M-4"/>
<gate name="-4" symbol="M-4"/>
</gates>
<devices>
<device name="047" package="53047-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="WALDOM/MOLEX"/>
<attribute name="MPN" value="53047-0410"/>
<attribute name="OC_FARNELL" value="9733060"/>
<attribute name="OC_NEWARK" value="38C9900"/>
</technology>
</technologies>
</device>
<device name="048" package="53048-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="53048-0410"/>
<attribute name="OC_FARNELL" value="1462887"/>
<attribute name="OC_NEWARK" value="57H4721"/>
</technology>
</technologies>
</device>
<device name="261" package="53261-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1125374"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="398" package="53398-04">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1125367"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>