<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="45.573" y2="0" width="0" layer="20"/>
<wire x1="45.573" y1="0" x2="45.573" y2="18.339" width="0" layer="20"/>
<wire x1="45.573" y1="18.339" x2="0" y2="18.339" width="0" layer="20"/>
<wire x1="0" y1="18.339" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="PiezoFFC">
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="70553-02">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Low Profile, Single Row, Right Angle, 3.05mm Pocket, Shrouded, 3 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705530002_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CAPC2012X130">
<description>Chip, 2.00 X 1.25 X 1.30 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.25 X 1.30 mm&lt;/p&gt;</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="PP-STANDALONE-HEADER">
<description>Double-row, 12-pin Receptacle Header (Female) Right Angle, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 7.36 mm insulator length, 15.24 X 7.36 X 5.56 mm body
&lt;p&gt;Double-row (2X6), 12-pin Receptacle Header (Female) Right Angle package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 7.36 mm insulator length with body size 15.24 X 7.36 X 5.56 mm, pin pattern - counter-clockwise from bottom left&lt;/p&gt;</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="PiezoFFC" package="SOT23" value="BAV199">
<attribute name="NAME"/>
</element>
<element name="C1" library="PiezoFFC" package="CAPC2012X130" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="PiezoFFC" package="SO14" value="LM2902D">
<attribute name="NAME"/>
</element>
<element name="PT1" library="PiezoFFC" package="70553-02" value="C-GRID-02-70553">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="C2" library="PiezoFFC" package="CAPC2012X130" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="PiezoFFC" package="CAPC2012X130" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="PiezoFFC" package="CAPC2012X130" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="PiezoFFC" package="CAPC2012X130" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="PiezoFFC" package="CAPC2012X130" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="PiezoFFC" package="CAPC2012X130" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="PiezoFFC" package="CAPC2012X130" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="PiezoFFC" package="CAPC2012X130" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="PiezoFFC" package="CAPC2012X130" value="3.3uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="PiezoFFC" package="CAPC2012X130" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="PiezoFFC" package="CAPC2012X130" value="3.3uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="PiezoFFC" package="PP-STANDALONE-HEADER" value="PP-STANDALONE-HEADER">
<attribute name="NAME"/>
</element>
<element name="PZ" library="PiezoFFC" package="70553-02" value="C-GRID-02-70553">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R10" library="PiezoFFC" package="R0805" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="PiezoFFC" package="R0805" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="PiezoFFC" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="PiezoFFC" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="PiezoFFC" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="PiezoFFC" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="PiezoFFC" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="PiezoFFC" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="PiezoFFC" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="PiezoFFC" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="PiezoFFC" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="PiezoFFC" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="PiezoFFC" package="R0805" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="PiezoFFC" package="R0805" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="PiezoFFC" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="PiezoFFC" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="PiezoFFC" package="R0805" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="PiezoFFC" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TRIG" library="PiezoFFC" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="PiezoFFC" package="R0805" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="J1" pad="7"/>
<contactref element="PZ" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="PWR" pad="C"/>
</signal>
<signal name="Z_TRG">
<contactref element="J1" pad="12"/>
<contactref element="R10" pad="2"/>
<contactref element="TRIG" pad="C"/>
</signal>
<signal name="PZ+">
<contactref element="D1" pad="3"/>
<contactref element="U1" pad="10"/>
<contactref element="PZ" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="D1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="GAIN_OUT1">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="R8" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="V_FOLLOW">
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="14"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="VCOMP_SENSE">
<contactref element="U1" pad="3"/>
<contactref element="C24" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="GADJ_R3">
<contactref element="J1" pad="5"/>
<contactref element="R7" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="PZ_AMP_OUT">
<contactref element="U1" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="AMP_VCC1">
<contactref element="U1" pad="4"/>
<contactref element="C19" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="PT_IN+1">
<contactref element="C2" pad="1"/>
<contactref element="PT1" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="PT_IN-1">
<contactref element="C4" pad="2"/>
<contactref element="PT1" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="PT_AMP-1">
<contactref element="C16" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="C18" pad="2"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="PT_AMP+1">
<contactref element="C16" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C17" pad="1"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="PT_AMP1">
<contactref element="U1" pad="7"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="GAIN_ADJ1">
<contactref element="U1" pad="9"/>
<contactref element="R6" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="V_FOL_ADJ1">
<contactref element="U1" pad="12"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="V_FOL_PWM">
<contactref element="J1" pad="9"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VCOMP_PWM">
<contactref element="J1" pad="8"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="GADJ_R2">
<contactref element="J1" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="GADJ_R1">
<contactref element="J1" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="GADJ_R0">
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="PT100_OUT">
<contactref element="C20" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="LED_VCC">
<contactref element="TRIG" pad="A"/>
<contactref element="R19" pad="1"/>
<contactref element="PWR" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
