<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<hole x="-8.765" y="15.493" drill="3.2"/>
<hole x="8.765" y="15.493" drill="3.2"/>
<hole x="9.034" y="-15.337" drill="3.2"/>
<hole x="-9.034" y="-15.337" drill="3.2"/>
<hole x="17.799" y="-0.155" drill="3.2"/>
<hole x="-17.799" y="-0.155" drill="3.2"/>
<wire x1="-24.75" y1="37.75" x2="24.75" y2="37.75" width="0.1524" layer="20" curve="-66.500033"/>
<wire x1="45" y1="3" x2="19.5" y2="-40.75" width="0.1524" layer="20" curve="-68.241673"/>
<wire x1="-19.5" y1="-40.75" x2="-45" y2="3" width="0.1524" layer="20" curve="-68.241673"/>
<wire x1="24.75" y1="37.75" x2="45" y2="3" width="0.1524" layer="20"/>
<wire x1="-24.75" y1="37.75" x2="-45" y2="3" width="0.1524" layer="20"/>
<wire x1="-19.5" y1="-40.75" x2="19.5" y2="-40.75" width="0.1524" layer="20"/>
<text>https://docs.pyroballpcbs.com</text>
<text>EzPz-Effector v2.3.1</text>
<wire x1="-20.6101" y1="-9.3014" x2="-20.6208" y2="-8.8734" width="0.1016" layer="20"/>
<wire x1="-20.6208" y1="-8.8734" x2="-20.5941" y2="-8.4461" width="0.1016" layer="20"/>
<wire x1="-20.5941" y1="-8.4461" x2="-20.5303" y2="-8.0228" width="0.1016" layer="20"/>
<wire x1="-20.5303" y1="-8.0228" x2="-20.4299" y2="-7.6066" width="0.1016" layer="20"/>
<wire x1="-20.4299" y1="-7.6066" x2="-20.2935" y2="-7.2007" width="0.1016" layer="20"/>
<wire x1="-20.2935" y1="-7.2007" x2="-20.1223" y2="-6.8083" width="0.1016" layer="20"/>
<wire x1="-20.1223" y1="-6.8083" x2="-19.9176" y2="-6.4323" width="0.1016" layer="20"/>
<wire x1="-19.9176" y1="-6.4323" x2="-19.6808" y2="-6.0756" width="0.1016" layer="20"/>
<wire x1="-19.6808" y1="-6.0756" x2="-19.4139" y2="-5.7409" width="0.1016" layer="20"/>
<wire x1="-19.4139" y1="-5.7409" x2="-19.1188" y2="-5.4307" width="0.1016" layer="20"/>
<wire x1="-19.1188" y1="-5.4307" x2="-18.7978" y2="-5.1474" width="0.1016" layer="20"/>
<wire x1="-18.7978" y1="-5.1474" x2="-18.4533" y2="-4.8931" width="0.1016" layer="20"/>
<wire x1="-18.4533" y1="-4.8931" x2="-18.0745" y2="-4.6621" width="0.1016" layer="20"/>
<wire x1="-18.0745" y1="-4.6621" x2="-16.2495" y2="-3.6084" width="0.1016" layer="20"/>
<wire x1="-16.2495" y1="-3.6084" x2="-13.9997" y2="-0.0976" width="0.1016" layer="20" curve="54.694"/>
<wire x1="-13.9997" y1="-0.0976" x2="-6.9158" y2="12.1726" width="0.1016" layer="20" curve="-60.7966"/>
<wire x1="-6.9158" y1="12.1726" x2="-5" y2="15.8767" width="0.1016" layer="20" curve="54.6966"/>
<wire x1="-5" y1="15.8767" x2="-5" y2="18" width="0.1016" layer="20"/>
<wire x1="-5" y1="18" x2="-4.9938" y2="18.2493" width="0.1016" layer="20" curve="-2.8579"/>
<wire x1="-4.9938" y1="18.2493" x2="-4.9893" y2="18.428" width="0.1016" layer="20"/>
<wire x1="-4.9893" y1="18.428" x2="-4.9414" y2="18.8535" width="0.1016" layer="20"/>
<wire x1="-4.9414" y1="18.8535" x2="-4.8565" y2="19.2731" width="0.1016" layer="20"/>
<wire x1="-4.8565" y1="19.2731" x2="-4.7354" y2="19.6837" width="0.1016" layer="20"/>
<wire x1="-4.7354" y1="19.6837" x2="-4.579" y2="20.0823" width="0.1016" layer="20"/>
<wire x1="-4.579" y1="20.0823" x2="-4.3885" y2="20.4657" width="0.1016" layer="20"/>
<wire x1="-4.3885" y1="20.4657" x2="-4.1652" y2="20.831" width="0.1016" layer="20"/>
<wire x1="-4.1652" y1="20.831" x2="-3.911" y2="21.1755" width="0.1016" layer="20"/>
<wire x1="-3.911" y1="21.1755" x2="-3.6277" y2="21.4965" width="0.1016" layer="20"/>
<wire x1="-3.6277" y1="21.4965" x2="-3.3175" y2="21.7916" width="0.1016" layer="20"/>
<wire x1="-3.3175" y1="21.7916" x2="-2.9827" y2="22.0585" width="0.1016" layer="20"/>
<wire x1="-2.9827" y1="22.0585" x2="-2.626" y2="22.2952" width="0.1016" layer="20"/>
<wire x1="-2.626" y1="22.2952" x2="-2.25" y2="22.5" width="0.1016" layer="20"/>
<wire x1="-2.25" y1="22.5" x2="-1.3742" y2="22.2791" width="0.1016" layer="20" curve="-44.7649"/>
<wire x1="-1.3742" y1="22.2791" x2="-1.234" y2="22.1428" width="0.1016" layer="20"/>
<wire x1="-1.234" y1="22.1428" x2="-1.1808" y2="22.0736" width="0.1016" layer="20"/>
<wire x1="-1.1808" y1="22.0736" x2="-1.134" y2="22" width="0.1016" layer="20"/>
<wire x1="-1.134" y1="22" x2="-1.0937" y2="21.9226" width="0.1016" layer="20"/>
<wire x1="-1.0937" y1="21.9226" x2="-1.0603" y2="21.842" width="0.1016" layer="20"/>
<wire x1="-1.0603" y1="21.842" x2="-1.0341" y2="21.7588" width="0.1016" layer="20"/>
<wire x1="-1.0341" y1="21.7588" x2="-1.0152" y2="21.6736" width="0.1016" layer="20"/>
<wire x1="-1.0152" y1="21.6736" x2="-1" y2="21.5" width="0.1016" layer="20"/>
<wire x1="-1" y1="21.5" x2="-1" y2="20.9361" width="0.1016" layer="20"/>
<wire x1="-1" y1="20.9361" x2="1" y2="20.9361" width="0.1016" layer="20" curve="290.3002"/>
<wire x1="1" y1="20.9361" x2="1" y2="21.5" width="0.1016" layer="20"/>
<wire x1="1" y1="21.5" x2="1.0152" y2="21.6736" width="0.1016" layer="20"/>
<wire x1="1.0152" y1="21.6736" x2="1.0341" y2="21.7588" width="0.1016" layer="20"/>
<wire x1="1.0341" y1="21.7588" x2="1.0603" y2="21.842" width="0.1016" layer="20"/>
<wire x1="1.0603" y1="21.842" x2="1.0937" y2="21.9226" width="0.1016" layer="20"/>
<wire x1="1.0937" y1="21.9226" x2="1.134" y2="22" width="0.1016" layer="20"/>
<wire x1="1.134" y1="22" x2="1.1808" y2="22.0736" width="0.1016" layer="20"/>
<wire x1="1.1808" y1="22.0736" x2="1.234" y2="22.1428" width="0.1016" layer="20"/>
<wire x1="1.234" y1="22.1428" x2="1.3742" y2="22.2791" width="0.1016" layer="20"/>
<wire x1="1.3742" y1="22.2791" x2="2.1794" y2="22.5" width="0.1016" layer="20" curve="-48.0969"/>
<wire x1="2.1794" y1="22.5" x2="2.626" y2="22.2952" width="0.1016" layer="20"/>
<wire x1="2.626" y1="22.2952" x2="2.9827" y2="22.0585" width="0.1016" layer="20"/>
<wire x1="2.9827" y1="22.0585" x2="3.3175" y2="21.7916" width="0.1016" layer="20"/>
<wire x1="3.3175" y1="21.7916" x2="3.6277" y2="21.4965" width="0.1016" layer="20"/>
<wire x1="3.6277" y1="21.4965" x2="3.911" y2="21.1755" width="0.1016" layer="20"/>
<wire x1="3.911" y1="21.1755" x2="4.1652" y2="20.831" width="0.1016" layer="20"/>
<wire x1="4.1652" y1="20.831" x2="4.3885" y2="20.4657" width="0.1016" layer="20"/>
<wire x1="4.3885" y1="20.4657" x2="4.579" y2="20.0823" width="0.1016" layer="20"/>
<wire x1="4.579" y1="20.0823" x2="4.7354" y2="19.6837" width="0.1016" layer="20"/>
<wire x1="4.7354" y1="19.6837" x2="4.8565" y2="19.2731" width="0.1016" layer="20"/>
<wire x1="4.8565" y1="19.2731" x2="4.9414" y2="18.8534" width="0.1016" layer="20"/>
<wire x1="4.9414" y1="18.8534" x2="4.9893" y2="18.428" width="0.1016" layer="20"/>
<wire x1="4.9893" y1="18.428" x2="4.9938" y2="18.2493" width="0.1016" layer="20"/>
<wire x1="4.9938" y1="18.2493" x2="5" y2="18" width="0.1016" layer="20" curve="-2.8584"/>
<wire x1="5" y1="18" x2="5" y2="15.8767" width="0.1016" layer="20"/>
<wire x1="5" y1="15.8767" x2="6.9158" y2="12.1726" width="0.1016" layer="20" curve="54.6966"/>
<wire x1="6.9158" y1="12.1726" x2="13.9997" y2="-0.0976" width="0.1016" layer="20" curve="-60.7966"/>
<wire x1="13.9997" y1="-0.0976" x2="14.0535" y2="-0.4899" width="0.1016" layer="20"/>
<wire x1="14.0535" y1="-0.4899" x2="16.2495" y2="-3.6084" width="0.1016" layer="20" curve="49.6942"/>
<wire x1="16.2495" y1="-3.6084" x2="18.2995" y2="-4.7991" width="0.1016" layer="20"/>
<wire x1="18.2995" y1="-4.7991" x2="18.4533" y2="-4.8931" width="0.1016" layer="20"/>
<wire x1="18.4533" y1="-4.8931" x2="18.7978" y2="-5.1474" width="0.1016" layer="20"/>
<wire x1="18.7978" y1="-5.1474" x2="19.1188" y2="-5.4307" width="0.1016" layer="20"/>
<wire x1="19.1188" y1="-5.4307" x2="19.4139" y2="-5.7409" width="0.1016" layer="20"/>
<wire x1="19.4139" y1="-5.7409" x2="19.6808" y2="-6.0756" width="0.1016" layer="20"/>
<wire x1="19.6808" y1="-6.0756" x2="19.9176" y2="-6.4323" width="0.1016" layer="20"/>
<wire x1="19.9176" y1="-6.4323" x2="20.1223" y2="-6.8083" width="0.1016" layer="20"/>
<wire x1="20.1223" y1="-6.8083" x2="20.2935" y2="-7.2007" width="0.1016" layer="20"/>
<wire x1="20.2935" y1="-7.2007" x2="20.4299" y2="-7.6066" width="0.1016" layer="20"/>
<wire x1="20.4299" y1="-7.6066" x2="20.5303" y2="-8.0228" width="0.1016" layer="20"/>
<wire x1="20.5303" y1="-8.0228" x2="20.5941" y2="-8.4461" width="0.1016" layer="20"/>
<wire x1="20.5941" y1="-8.4461" x2="20.6208" y2="-8.8734" width="0.1016" layer="20"/>
<wire x1="20.6208" y1="-8.8734" x2="20.6101" y2="-9.3014" width="0.1016" layer="20"/>
<wire x1="20.6101" y1="-9.3014" x2="19.9772" y2="-9.951" width="0.1016" layer="20" curve="-45.2618"/>
<wire x1="19.9772" y1="-9.951" x2="19.7927" y2="-10.0028" width="0.1016" layer="20"/>
<wire x1="19.7927" y1="-10.0028" x2="19.7062" y2="-10.0141" width="0.1016" layer="20"/>
<wire x1="19.7062" y1="-10.0141" x2="19.6191" y2="-10.0179" width="0.1016" layer="20"/>
<wire x1="19.6191" y1="-10.0179" x2="19.5319" y2="-10.0141" width="0.1016" layer="20"/>
<wire x1="19.5319" y1="-10.0141" x2="19.4454" y2="-10.0028" width="0.1016" layer="20"/>
<wire x1="19.4454" y1="-10.0028" x2="19.3603" y2="-9.9839" width="0.1016" layer="20"/>
<wire x1="19.3603" y1="-9.9839" x2="19.2771" y2="-9.9576" width="0.1016" layer="20"/>
<wire x1="19.2771" y1="-9.9576" x2="19.1965" y2="-9.9243" width="0.1016" layer="20"/>
<wire x1="19.1965" y1="-9.9243" x2="18.6312" y2="-9.602" width="0.1016" layer="20"/>
<wire x1="18.6312" y1="-9.602" x2="16.0164" y2="-8.2321" width="0.1016" layer="20" curve="115"/>
<wire x1="16.0164" y1="-8.2321" x2="17.6312" y2="-11.3341" width="0.1016" layer="20" curve="175.3002"/>
<wire x1="17.6312" y1="-11.3341" x2="18.1195" y2="-11.616" width="0.1016" layer="20"/>
<wire x1="18.1195" y1="-11.616" x2="18.2619" y2="-11.716" width="0.1016" layer="20"/>
<wire x1="18.2619" y1="-11.716" x2="18.3262" y2="-11.7749" width="0.1016" layer="20"/>
<wire x1="18.3262" y1="-11.7749" x2="18.3851" y2="-11.8393" width="0.1016" layer="20"/>
<wire x1="18.3851" y1="-11.8393" x2="18.4382" y2="-11.9085" width="0.1016" layer="20"/>
<wire x1="18.4382" y1="-11.9085" x2="18.4851" y2="-11.9821" width="0.1016" layer="20"/>
<wire x1="18.4851" y1="-11.9821" x2="18.5254" y2="-12.0594" width="0.1016" layer="20"/>
<wire x1="18.5254" y1="-12.0594" x2="18.5588" y2="-12.14" width="0.1016" layer="20"/>
<wire x1="18.5588" y1="-12.14" x2="18.6054" y2="-12.3195" width="0.1016" layer="20"/>
<wire x1="18.6054" y1="-12.3195" x2="18.3601" y2="-13.1986" width="0.1016" layer="20" curve="-48.6754"/>
<wire x1="18.3601" y1="-13.1986" x2="17.9948" y2="-13.4218" width="0.1016" layer="20"/>
<wire x1="17.9948" y1="-13.4218" x2="17.6114" y2="-13.6124" width="0.1016" layer="20"/>
<wire x1="17.6114" y1="-13.6124" x2="17.2129" y2="-13.7688" width="0.1016" layer="20"/>
<wire x1="17.2129" y1="-13.7688" x2="16.8022" y2="-13.8899" width="0.1016" layer="20"/>
<wire x1="16.8022" y1="-13.8899" x2="16.3826" y2="-13.9747" width="0.1016" layer="20"/>
<wire x1="16.3826" y1="-13.9747" x2="15.9571" y2="-14.0227" width="0.1016" layer="20"/>
<wire x1="15.9571" y1="-14.0227" x2="15.5291" y2="-14.0334" width="0.1016" layer="20"/>
<wire x1="15.5291" y1="-14.0334" x2="15.1018" y2="-14.0067" width="0.1016" layer="20"/>
<wire x1="15.1018" y1="-14.0067" x2="14.6784" y2="-13.9429" width="0.1016" layer="20"/>
<wire x1="14.6784" y1="-13.9429" x2="14.2623" y2="-13.8424" width="0.1016" layer="20"/>
<wire x1="14.2623" y1="-13.8424" x2="13.8564" y2="-13.7061" width="0.1016" layer="20"/>
<wire x1="13.8564" y1="-13.7061" x2="13.464" y2="-13.5349" width="0.1016" layer="20"/>
<wire x1="13.464" y1="-13.5349" x2="13.306" y2="-13.4488" width="0.1016" layer="20"/>
<wire x1="13.306" y1="-13.4488" x2="13.088" y2="-13.3301" width="0.1016" layer="20" curve="-2.8442"/>
<wire x1="13.088" y1="-13.3301" x2="11.2124" y2="-12.2472" width="0.1016" layer="20"/>
<wire x1="11.2124" y1="-12.2472" x2="7.3877" y2="-11.9489" width="0.1016" layer="20" curve="50.0001"/>
<wire x1="7.3877" y1="-11.9489" x2="7.0839" y2="-12.0755" width="0.1016" layer="20"/>
<wire x1="7.0839" y1="-12.0755" x2="-7.0839" y2="-12.0755" width="0.1016" layer="20" curve="-60.7949"/>
<wire x1="-7.0839" y1="-12.0755" x2="-7.4505" y2="-11.9259" width="0.1016" layer="20"/>
<wire x1="-7.4505" y1="-11.9259" x2="-11.2099" y2="-12.2458" width="0.1016" layer="20" curve="49.1194"/>
<wire x1="-11.2099" y1="-12.2458" x2="-13.088" y2="-13.3301" width="0.1016" layer="20"/>
<wire x1="-13.088" y1="-13.3301" x2="-13.3059" y2="-13.4488" width="0.1016" layer="20" curve="-2.8429"/>
<wire x1="-13.3059" y1="-13.4488" x2="-13.464" y2="-13.5349" width="0.1016" layer="20"/>
<wire x1="-13.464" y1="-13.5349" x2="-13.8564" y2="-13.7061" width="0.1016" layer="20"/>
<wire x1="-13.8564" y1="-13.7061" x2="-14.2623" y2="-13.8424" width="0.1016" layer="20"/>
<wire x1="-14.2623" y1="-13.8424" x2="-14.6785" y2="-13.9429" width="0.1016" layer="20"/>
<wire x1="-14.6785" y1="-13.9429" x2="-15.1018" y2="-14.0067" width="0.1016" layer="20"/>
<wire x1="-15.1018" y1="-14.0067" x2="-15.5291" y2="-14.0334" width="0.1016" layer="20"/>
<wire x1="-15.5291" y1="-14.0334" x2="-15.9571" y2="-14.0227" width="0.1016" layer="20"/>
<wire x1="-15.9571" y1="-14.0227" x2="-16.3826" y2="-13.9747" width="0.1016" layer="20"/>
<wire x1="-16.3826" y1="-13.9747" x2="-16.8022" y2="-13.8899" width="0.1016" layer="20"/>
<wire x1="-16.8022" y1="-13.8899" x2="-17.2129" y2="-13.7688" width="0.1016" layer="20"/>
<wire x1="-17.2129" y1="-13.7688" x2="-17.6114" y2="-13.6124" width="0.1016" layer="20"/>
<wire x1="-17.6114" y1="-13.6124" x2="-17.9948" y2="-13.4218" width="0.1016" layer="20"/>
<wire x1="-17.9948" y1="-13.4218" x2="-18.3601" y2="-13.1986" width="0.1016" layer="20"/>
<wire x1="-18.3601" y1="-13.1986" x2="-18.6054" y2="-12.3195" width="0.1016" layer="20" curve="-45.5838"/>
<wire x1="-18.6054" y1="-12.3195" x2="-18.5588" y2="-12.14" width="0.1016" layer="20"/>
<wire x1="-18.5588" y1="-12.14" x2="-18.5254" y2="-12.0594" width="0.1016" layer="20"/>
<wire x1="-18.5254" y1="-12.0594" x2="-18.4851" y2="-11.9821" width="0.1016" layer="20"/>
<wire x1="-18.4851" y1="-11.9821" x2="-18.4382" y2="-11.9085" width="0.1016" layer="20"/>
<wire x1="-18.4382" y1="-11.9085" x2="-18.3851" y2="-11.8393" width="0.1016" layer="20"/>
<wire x1="-18.3851" y1="-11.8393" x2="-18.3262" y2="-11.7749" width="0.1016" layer="20"/>
<wire x1="-18.3262" y1="-11.7749" x2="-18.2619" y2="-11.716" width="0.1016" layer="20"/>
<wire x1="-18.2619" y1="-11.716" x2="-18.1195" y2="-11.616" width="0.1016" layer="20"/>
<wire x1="-18.1195" y1="-11.616" x2="-17.6312" y2="-11.3341" width="0.1016" layer="20"/>
<wire x1="-17.6312" y1="-11.3341" x2="-18.6312" y2="-9.602" width="0.1016" layer="20" curve="290.3002"/>
<wire x1="-18.6312" y1="-9.602" x2="-19.1965" y2="-9.9243" width="0.1016" layer="20"/>
<wire x1="-19.1965" y1="-9.9243" x2="-19.2771" y2="-9.9576" width="0.1016" layer="20"/>
<wire x1="-19.2771" y1="-9.9576" x2="-19.3603" y2="-9.9839" width="0.1016" layer="20"/>
<wire x1="-19.3603" y1="-9.9839" x2="-19.4454" y2="-10.0028" width="0.1016" layer="20"/>
<wire x1="-19.4454" y1="-10.0028" x2="-19.5319" y2="-10.0141" width="0.1016" layer="20"/>
<wire x1="-19.5319" y1="-10.0141" x2="-19.6191" y2="-10.0179" width="0.1016" layer="20"/>
<wire x1="-19.6191" y1="-10.0179" x2="-19.7062" y2="-10.0141" width="0.1016" layer="20"/>
<wire x1="-19.7062" y1="-10.0141" x2="-19.7927" y2="-10.0028" width="0.1016" layer="20"/>
<wire x1="-19.7927" y1="-10.0028" x2="-19.9772" y2="-9.951" width="0.1016" layer="20"/>
<wire x1="-19.9772" y1="-9.951" x2="-20.6101" y2="-9.3014" width="0.1016" layer="20" curve="-48.3492"/>
<text>DTR 

RXD

TXD

GND

+5V</text>
<text>MISO  +5V

SCK   MOSI

RST    GND</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP06R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="PiezoFFC">
<packages>
<package name="DO-219AC">
</package>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SEEED-RESISTOR_R0603">
</package>
<package name="0606_LED">
<description>&lt;h3&gt;0606 - LED SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.8mm&lt;/li&gt;
&lt;li&gt;Area:1.6mm L x 1.5mm W&lt;/li&gt;
&lt;li&gt;Height: 0.55m&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://optoelectronics.liteon.com/upload/download/DS22-2000-282/P_100_LTST-C195KGJRKT.pdf"&gt;LTST-C195KGJRKT&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LTST-C195KGJRKT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SEEED-LED_LED-0603">
</package>
<package name="HDRVR5W64P254_1X5_1270X254X575B">
<description>Single-row, 5-pin Receptacle Header (Female) Straight, 2.54 mm (0.10 in) col pitch, 5.75 mm insulator length, 12.70 X 2.54 X 5.75 mm body
&lt;p&gt;Single-row (1X5), 5-pin Receptacle Header (Female) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.75 mm insulator length with overall size 12.70 X 2.54 X 5.75 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="ICSP_3X2_2.54_STRAIGHT">
<description>Three-row, 6-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 5.08 X 7.62 X 8.38 mm body
&lt;p&gt;Three-row (3X2), 6-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.84 mm mating length with overall size 5.08 X 7.62 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="70543-06">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Single Row, Vertical, 3.05mm Pocket, Shrouded, 7 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705430006_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="EFFECTOR-45MM-ROD">
</package>
<package name="QFP80P900X900X120-32N">
</package>
<package name="SSOP14">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="70543-02">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Single Row, Vertical, 3.05mm Pocket, Shrouded, 3 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705430002_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="PIEZO-DISK-12MM-OFFSET">
</package>
<package name="SOT230P700X180-4N">
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="ALU-C-D5.3MM_RIGHT">
</package>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="5566-4">
<description>&lt;b&gt;Mini-Fit Jr.™ Vertical Header, 4.20mm Pitch, Dual Row, 4 Circuits, without Snap-in Plastic Peg PCB Lock, Tin, Natural&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/039281043_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="70543-04">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Single Row, Vertical, 3.05mm Pocket, Shrouded, 5 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705430004_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="LOGO-PYR0BALL-SS-20MM">
</package>
<package name="LOGO-PYR0BALL-SS-6MM">
</package>
<package name="OSHW_8MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="PiezoFFC" package="C0603K" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="PiezoFFC" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="PiezoFFC" package="C0603K" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="PiezoFFC" package="C0603K" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="PiezoFFC" package="C0603K" value="3.3uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="PiezoFFC" package="C0603K" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="PiezoFFC" package="C0603K" value="3.3uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="PiezoFFC" package="ALU-C-D5.3MM_RIGHT" value="100uf">
<attribute name="NAME"/>
</element>
<element name="C3" library="PiezoFFC" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="PiezoFFC" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="PiezoFFC" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="PiezoFFC" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="PiezoFFC" package="C0603K" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="PiezoFFC" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="PiezoFFC" package="C0603K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="PiezoFFC" package="DO-219AC" value="DIODE_ZENER_PLZ5V1C"/>
<element name="D8" library="PiezoFFC" package="SOT23" value="BAV199">
<attribute name="NAME"/>
</element>
<element name="INT" library="testpad" package="TP06R" value="TPTP06R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="PiezoFFC" package="0606_LED" value="LED-RGB-COM_ANO0606">
<attribute name="PROD_ID" value="DIO-12140"/>
</element>
<element name="RDY" library="PiezoFFC" package="SEEED-LED_LED-0603" value="">
<attribute name="NAME"/>
</element>
<element name="SJ1" library="PiezoFFC" package="SJ" value="">
<attribute name="NAME"/>
</element>
<element name="U2" library="PiezoFFC" package="SOT230P700X180-4N" value="LM317DCYSOT223">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" IC Regulator LM317/SOT223/LM317DCY TEXAS INSTRUMENT RoHS Ampere=1.5 SOT223 "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="LM317DCY"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-223-4 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="U3" library="PiezoFFC" package="SSOP14" value="LM2902PT">
<attribute name="NAME"/>
</element>
<element name="UART" library="PiezoFFC" package="HDRVR5W64P254_1X5_1270X254X575B" value="JST-2.54MM_5P-2.54JST_2.54MM_5P_F">
<attribute name="NAME"/>
</element>
<element name="ICSP" library="PiezoFFC" package="ICSP_3X2_2.54_STRAIGHT" value="ICSP_HEADERICSP-2.54MM">
<attribute name="NAME"/>
</element>
<element name="J1" library="PiezoFFC" package="70543-06" value="C-GRID-06-70543">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="H1" library="PiezoFFC" package="EFFECTOR-45MM-ROD" value="EFFECTOR-ROD-MOUNT">
<attribute name="NAME"/>
</element>
<element name="H2" library="PiezoFFC" package="EFFECTOR-45MM-ROD" value="EFFECTOR-ROD-MOUNT">
<attribute name="NAME"/>
</element>
<element name="H3" library="PiezoFFC" package="EFFECTOR-45MM-ROD" value="EFFECTOR-ROD-MOUNT">
<attribute name="NAME"/>
</element>
<element name="U1" library="PiezoFFC" package="QFP80P900X900X120-32N" value="ATMEGA328PTQFP-32">
<attribute name="NAME"/>
</element>
<element name="PT100" library="PiezoFFC" package="70543-02" value="C-GRID-02-70543">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="PZ1" library="PiezoFFC" package="PIEZO-DISK-12MM-OFFSET" value="PIEZO-DISK12MM-OFFSET"/>
<element name="PZ2" library="PiezoFFC" package="PIEZO-DISK-12MM-OFFSET" value="PIEZO-DISK12MM-OFFSET"/>
<element name="PZ3" library="PiezoFFC" package="PIEZO-DISK-12MM-OFFSET" value="PIEZO-DISK12MM-OFFSET"/>
<element name="R11" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="3K6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="3K3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="3K3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="PiezoFFC" package="SEEED-RESISTOR_R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="PiezoFFC" package="C0603K" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V/TH_IN" library="PiezoFFC" package="5566-4" value="5566-4">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="1"/>
</element>
<element name="HEATER" library="PiezoFFC" package="70543-04" value="C-GRID-04-70543">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="U$1" library="PiezoFFC" package="LOGO-PYR0BALL-SS-20MM" value=""/>
<element name="U$2" library="PiezoFFC" package="LOGO-PYR0BALL-SS-6MM" value=""/>
<element name="U$3" library="PiezoFFC" package="LOGO-PYR0BALL-SS-6MM" value=""/>
<element name="U$4" library="PiezoFFC" package="LOGO-PYR0BALL-SS-6MM" value=""/>
<element name="U$5" library="PiezoFFC" package="OSHW_8MM" value=""/>
<element name="U$6" library="PiezoFFC" package="OSHW_8MM" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="P$1"/>
<contactref element="C4" pad="1"/>
<contactref element="LED" pad="P$3"/>
<contactref element="RDY" pad="-"/>
<contactref element="U3" pad="11"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="D8" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="H1" pad="P$1"/>
<contactref element="H1" pad="P$2"/>
<contactref element="H2" pad="P$1"/>
<contactref element="H2" pad="P$2"/>
<contactref element="H3" pad="P$1"/>
<contactref element="H3" pad="P$2"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="UART" pad="2"/>
<contactref element="ICSP" pad="6"/>
<contactref element="PZ1" pad="GND2"/>
<contactref element="PZ1" pad="GND1"/>
<contactref element="PZ1" pad="GND3"/>
<contactref element="PZ2" pad="GND2"/>
<contactref element="PZ2" pad="GND1"/>
<contactref element="PZ2" pad="GND3"/>
<contactref element="PZ3" pad="GND2"/>
<contactref element="PZ3" pad="GND1"/>
<contactref element="PZ3" pad="GND3"/>
<contactref element="R11" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="C2" pad="-"/>
</signal>
<signal name="Z_MIN_TRIG">
<contactref element="LED" pad="P$4"/>
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="11"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="VCC_REG">
<contactref element="J1" pad="4"/>
<contactref element="F1" pad="1"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="TTL_RXD">
<contactref element="U1" pad="30"/>
<contactref element="UART" pad="4"/>
</signal>
<signal name="TTL_TXD">
<contactref element="U1" pad="31"/>
<contactref element="UART" pad="3"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="29"/>
<contactref element="ICSP" pad="5"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="SPI_SCK">
<contactref element="U1" pad="17"/>
<contactref element="ICSP" pad="4"/>
</signal>
<signal name="SPI_MISO">
<contactref element="U1" pad="16"/>
<contactref element="ICSP" pad="1"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="U1" pad="15"/>
<contactref element="ICSP" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="SCL">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="Z_TRG">
<contactref element="INT" pad="TP"/>
<contactref element="U1" pad="32"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="PZ+">
<contactref element="D8" pad="3"/>
<contactref element="U3" pad="10"/>
<contactref element="PZ1" pad="PZ+"/>
<contactref element="PZ2" pad="PZ+"/>
<contactref element="PZ3" pad="PZ+"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="P$2"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="SJ1" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="UART" pad="1"/>
<contactref element="ICSP" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="GAIN_OUT">
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="V_FOLLOW">
<contactref element="U3" pad="13"/>
<contactref element="U3" pad="14"/>
<contactref element="U1" pad="23"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="VCOMP_SENSE">
<contactref element="U3" pad="3"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U1" pad="24"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="GADJ_R0">
<contactref element="U1" pad="7"/>
<contactref element="R14" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="GADJ_R1">
<contactref element="U1" pad="8"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="GADJ_R2">
<contactref element="U1" pad="9"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="GADJ_R3">
<contactref element="U1" pad="10"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="PZ_AMP_OUT">
<contactref element="U3" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="ERR_LED">
<contactref element="LED" pad="P$1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="VCC_FUSE">
<contactref element="SJ1" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="AMP_VCC">
<contactref element="U3" pad="4"/>
<contactref element="C10" pad="2"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="PT_IN+">
<contactref element="C5" pad="1"/>
<contactref element="PT100" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="PT_IN-">
<contactref element="C6" pad="2"/>
<contactref element="PT100" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="PT_AMP-">
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="6"/>
<contactref element="C9" pad="2"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="PT_AMP+">
<contactref element="C7" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="C8" pad="1"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="PT_AMP">
<contactref element="U3" pad="7"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="PT100_OUT">
<contactref element="J1" pad="6"/>
<contactref element="C11" pad="2"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="GAIN_ADJ">
<contactref element="U3" pad="9"/>
<contactref element="R16" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="V_FOL_ADJ">
<contactref element="U3" pad="12"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="V_FOL_PWM">
<contactref element="U1" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="VCOMP_PWM">
<contactref element="U1" pad="13"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="LED_PWR">
<contactref element="LED" pad="P$2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="RDY_LED">
<contactref element="RDY" pad="+"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="PZ_DET">
<contactref element="U1" pad="25"/>
</signal>
<signal name="REG_ADJ">
<contactref element="U2" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VCC_ADJ">
<contactref element="U1" pad="12"/>
<contactref element="R9" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="TTL_DTR">
<contactref element="UART" pad="5"/>
<contactref element="C16" pad="2"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="VIN_12/24">
<contactref element="V/TH_IN" pad="4"/>
<contactref element="HEATER" pad="1"/>
</signal>
<signal name="TH1">
<contactref element="V/TH_IN" pad="3"/>
<contactref element="HEATER" pad="2"/>
</signal>
<signal name="TH0">
<contactref element="HEATER" pad="3"/>
<contactref element="V/TH_IN" pad="1"/>
</signal>
<signal name="HE0-">
<contactref element="HEATER" pad="4"/>
<contactref element="V/TH_IN" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
